;*****************************************************************************
;*
;*  l1ce51x86.INF  -   Atheros AR813X/AR815X Series PCI-E Ethernet Controller
;*  Copyright 2005-, Atheros Co., Ltd.
;*
;*****************************************************************************
[Version]
Signature   = "$WINDOWS NT$"
Class       = Net
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Provider    = %Atheros%
CatalogFile = l1c51x86.cat
Compatible  = 1
DriverVer   = 03/22/2011,1.0.1.47

[Manufacturer]
%Atheros% = Atheros

[Atheros]
; DisplayName           Section         	    DeviceID
; -----------           -------         	    --------
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063                         ; L1C
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_10631969&REV_C0

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_83041043&REV_C0  ; ASUS
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_83FE1043&REV_C0  ; ASUS
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_84921043&REV_C0  ; ASUS
%Atheros.L1c%   =       L1c.DisS5.ndi,              PCI\VEN_1969&DEV_1063&SUBSYS_18201043&REV_C0  ; ASUS
%Atheros.L1c%   =       L1c.DisS5.ndi,              PCI\VEN_1969&DEV_1063&SUBSYS_18301043&REV_C0  ; ASUS

%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_20081854&REV_C0  ; Pegatron
%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_20091854&REV_C0  ; Pegatron
%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_FF101854&REV_C0  ; Pegatron
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_202F1B0A&REV_C0  ; Pegatron
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_00C31B0A&REV_C0  ; Pegatron
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_00C91B0A&REV_C0  ; Pegatron

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_10D217C0&REV_C0  ; M10B1
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_10D717C0&REV_C0  ; Dagger

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_394E17AA&REV_C0  ; NAUR2,NAWA
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_395817AA&REV_C0  ; NIMUA/B
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_395617AA&REV_C0  ; LU16_INTEL
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_396117AA&REV_C0  ; LU16_AMD

%Atheros.L1c%   =       L1c.GIGABYTE.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_E0001458&REV_C0  ; GIGABYTE

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_81311019&REV_C0  ; ECS

%Atheros.L1c%   =       L1c.Toshiba.ndi,            PCI\VEN_1969&DEV_1063&SUBSYS_FF501179&REV_C0  ; TZ2

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02291025&REV_C0  ; JM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_027F1025&REV_C0  ; JM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02801025&REV_C0  ; JM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02381025&REV_C0  ; SJM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02811025&REV_C0  ; SJM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02821025&REV_C0  ; SJM31
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_03021025&REV_C0  ; SJM52
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_03031025&REV_C0  ; SJM52
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_03041025&REV_C0  ; SJM52
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_022A1025&REV_C0  ; JM41
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_022B1025&REV_C0  ; JM51
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_034B1025&REV_C0  ; NCL20
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04301025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04311025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04321025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04331025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04341025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04111025&REV_C0  ; NCWH1
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041C1025&REV_C0  ; SJM30
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041D1025&REV_C0  ; SJM30
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_042B1025&REV_C0  ; SJM50
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_042C1025&REV_C0  ; SJM30
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04201025&REV_C0  ; SJM50NP_UMA
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04211025&REV_C0  ; SJM50NP_UMA
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041E1025&REV_C0  ; SJM50CP_UMA
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041F1025&REV_C0  ; SJM50CP_DIS
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_04501025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_044F1025&REV_C0  ; SJM40
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_049B1025&REV_C0  ; HM55_MV

%Atheros.L1c%   =       L1c.SONY.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_390217AA&REV_C0  ; LU15
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_395617AA&REV_C0  ; LA46

%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_01671025&REV_C0  ; KAL90
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_021B1025&REV_C0  ; KBLG0
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_02601025&REV_C0  ; KALG0
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_027D1025&REV_C0  ; NBLG0
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_01281025&REV_C0  ; KALH0

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_004214C0&REV_C0  ; NBLB1
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_004314C0&REV_C0  ; NBLB2
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_004514C0&REV_C0  ; NTTB1
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_004614C0&REV_C0  ; NTUC0

%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_021E1025&REV_C0  ; ZK6
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_02531025&REV_C0  ; ZR6
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_026A1025&REV_C0  ; ZK8
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_026D1025&REV_C0  ; ZK8
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_026E1025&REV_C0  ; ZK8
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_029B1025&REV_C0  ; ZH7
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_029F1025&REV_C0  ; ZH8
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_029E1025&REV_C0  ; ZH6
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_03001025&REV_C0  ; ZE8
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_029D1025&REV_C0  ; ZE9
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_03321025&REV_C0  ; ZH9

%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_7009103C&REV_C0  ; SP7
%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_1522103C&REV_C0  ; Nikita
%Atheros.L1c%   =       L1c.ShutOn.ndi,             PCI\VEN_1969&DEV_1063&SUBSYS_147D103C&REV_C0  ; Nikita1.2

%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1411103C&REV_C0  ; ZENO
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1412103C&REV_C0  ; ZENO
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1413103C&REV_C0  ; ZENO
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_142C103C&REV_C0  ; PETEK
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_142D103C&REV_C0  ; PETEK
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1421103C&REV_C0  ; Hamilton
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1423103C&REV_C0  ; Hamilton
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_1420103C&REV_C0  ; Prano
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_142B103C&REV_C0  ; Prano

%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0D4E105B&REV_C0  ; AJ-BOX
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0D52105B&REV_C0  ; AJ-BOX-N
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0CD9105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0D56105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0CDA105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0E35105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0D57105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0CFC105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0CFD105B&REV_C0  ; Clone
%Atheros.L1c%   =       L1c.ShutOn.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_0DC5105B&REV_C0  ; Clone

%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_07991854&REV_C0  ; QL2
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08001854&REV_C0  ; QL2
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08031854&REV_C0  ; QL4
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08041854&REV_C0  ; QL4
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08051854&REV_C0  ; QL2
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08071854&REV_C0  ; QL4
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08211854&REV_C0  ; QL4
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_08321854&REV_C0  ; QL4
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_20101854&REV_C0  ; PEGATRON
%Atheros.L1c%   =       L1c.ndi,        	    PCI\VEN_1969&DEV_1063&SUBSYS_20111854&REV_C0  ; PEGATRON

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0809152D&REV_C0  ; SW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0810152D&REV_C0  ; SW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0812152D&REV_C0  ; TW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0813152D&REV_C0  ; TW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0814152D&REV_C0  ; SW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0815152D&REV_C0  ; TW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0822152D&REV_C0  ; TW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0828152D&REV_C0  ; TW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0831152D&REV_C0  ; TW9A
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0835152D&REV_C0  ; SW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0852152D&REV_C0  ; TW9D
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0853152D&REV_C0  ; TW9D
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0854152D&REV_C0  ; TW9E
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0855152D&REV_C0  ; SW9
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_0856152D&REV_C0  ; SW9D

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041E1028&REV_C0  ; Dell-DC1
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_041F1028&REV_C0  ; Dell-DC2

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_906A104D&REV_C0  ; NEO
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_9069104D&REV_C0  ; NEO
%Atheros.L1c%   =       L1c.SONY.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_906F104D&REV_C0  ; Sony
%Atheros.L1c%   =       L1c.SONY.ndi,               PCI\VEN_1969&DEV_1063&SUBSYS_9076104D&REV_C0  ; Cadiz
%Atheros.L1c%   =       L1c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1063&SUBSYS_906C104D&REV_C0  ; TW6
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_907C104D&REV_C0  ; Tucana
%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_9082104D&REV_C0  ; Tucana-BR

%Atheros.L1c%   =       L1c.ndi,                    PCI\VEN_1969&DEV_1063&SUBSYS_10D217C0&REV_C0  ; M10B1

%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062	                  ; L2C
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_10621969&REV_C0

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_83041043&REV_C0  ; ASUS
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_83FF1043&REV_C0  ; ASUS
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_838A1043&REV_C0  ; EEEPC
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_83BE1043&REV_C0  ; EEEPC
%Atheros.L2c%   =       L2c.DisS5.ndi,              PCI\VEN_1969&DEV_1062&SUBSYS_14E51043&REV_C0  ; F50Q
%Atheros.L2c%   =       L2c.DisS5.ndi,              PCI\VEN_1969&DEV_1062&SUBSYS_15251043&REV_C0  ; ASUS

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_81321019&REV_C0  ; ECS

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_20261B0A&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_1598103C&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.WOLMagic.ndi,           PCI\VEN_1969&DEV_1062&SUBSYS_00AA1B0A&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_20081854&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_20091854&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_200A1854&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_200B1854&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_200D1854&REV_C0  ; PEGATRON, H00J
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_200E1854&REV_C0  ; PEGATRON
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_00E01B0A&REV_C0  ; PEGATRON

%Atheros.L2c%   =       L2c.GIGABYTE.ndi,           PCI\VEN_1969&DEV_1062&SUBSYS_E0001458&REV_C0  ; GIGABYTE

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_394F17AA&REV_C0  ; NAUR2,NAWA
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_38A317AA&REV_C0  ; LA14
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_395617AA&REV_C0  ; LA46
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_395817AA&REV_C0  ; NIMUA/B

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_019C1025&REV_C0  ; KAV10
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02101025&REV_C0  ; KAWH0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02111025&REV_C0  ; KBWH0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02121025&REV_C0  ; KAWF0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02131025&REV_C0  ; KAWG0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02141025&REV_C0  ; HM40-MV
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02151025&REV_C0  ; HM40-YK
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02161025&REV_C0  ; HM20-YK
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_019D1025&REV_C0  ;
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_022E1025&REV_C0  ; KAW10
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_022F1025&REV_C0  ; KAV50
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_02301025&REV_C0  ; KAV60
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_02411025&REV_C0  ; KAV80
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_02431025&REV_C0  ; KAVA0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_02601025&REV_C0  ; KALG0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_028D1025&REV_C0  ; HM50/70-PU
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_03491025&REV_C0  ; NAV50
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_034A1025&REV_C0  ; NAV60
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_030D1025&REV_C0  ; HM41
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_03501025&REV_C0  ; HM50/51/70
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04111025&REV_C0  ; NCWH1
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04391025&REV_C0  ; NAVD0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_043A1025&REV_C0  ; NAVD0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_043B1025&REV_C0  ; NAVE0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_043C1025&REV_C0  ; NAVE0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04591025&REV_C0  ; JE50_MV
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_045A1025&REV_C0  ; HM52_MV
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_045B1025&REV_C0  ; BA51_MV
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04971025&REV_C0  ; PAV50

%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_308F103C&REV_C0  ; BIXBY
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_1468103C&REV_C0  ; BIXBY 2.0
%Atheros.L2c%   =       L2c.ShutOn.ndi,             PCI\VEN_1969&DEV_1062&SUBSYS_1492103C         ;

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_0820152D&REV_C0  ; UW2

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04091028&REV_C0  ; ARGOS
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04431028&REV_C0  ; Phantom
%Atheros.L2c%   =       L2c.ndi,               	    PCI\VEN_1969&DEV_1062&SUBSYS_04511028&REV_C0  ; DJ
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04521028&REV_C0  ; DJ
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04531028&REV_C0  ; DJ
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04541028&REV_C0  ; DJ
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04651028&REV_C0  ; NAP10
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04661028&REV_C0  ; DJx
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04701028&REV_C0  ; NLM01
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04711028&REV_C0  ; NLM00
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_046F1028&REV_C0  ; DJ1_AMD
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04A61028&REV_C0  ; DJ2_MV
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_049E1028&REV_C0  ; DJ2_AMD
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_049F1028&REV_C0  ; DJ2_CP_UMA
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_04A01028&REV_C0  ; DJ2_CP_DIS

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_004414C0&REV_C0  ; NTTB0
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_004714C0&REV_C0  ; NTV00/10

%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_022C1025&REV_C0  ; ZG8
%Atheros.L2c%   =       L2c.Toshiba.ndi,            PCI\VEN_1969&DEV_1062&SUBSYS_FF501179&REV_C0  ; TZ2
%Atheros.L2c%   =       L2c.Toshiba.ndi,            PCI\VEN_1969&DEV_1062&SUBSYS_FFE01179&REV_C0  ; BU3
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_022C1025&REV_C0  ; ZG8
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_0790152D&REV_C0  ; IN1
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_02441025&REV_C0  ; ZA3
%Atheros.L2c%   =       L2c.ndi,        	    PCI\VEN_1969&DEV_1062&SUBSYS_9064104D&REV_C0  ; SY2
%Atheros.L2c%   =       L2c.ndi,                    PCI\VEN_1969&DEV_1062&SUBSYS_9066104D&REV_C0  ; SY3

%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060	                  ; L2cB
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_20601969&REV_C1  ; L2cB

%Atheros.L2cb%  =       L2cb.PWMAll.ndi,            PCI\VEN_1969&DEV_2060&SUBSYS_FF1E1179&REV_C1  ; IEC
%Atheros.L2cb%  =       L2cb.PWMAll.ndi,            PCI\VEN_1969&DEV_2060&SUBSYS_FDD01179&REV_C1  ; TE6

%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04511028&REV_C1  ; DJ1_MV
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04551028&REV_C1  ; UM7
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04561028&REV_C1  ; UM8
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04571028&REV_C1  ; UM9
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_04661028&REV_C1  ; DJ1_CP
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_046F1028&REV_C1  ; DJ1_AMD
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04861028&REV_C1  ; DJ2_CP
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_04871028&REV_C1  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_048F1028&REV_C1  ; Dell_Avenger
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04901028&REV_C1  ; Dell_Voyager
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04A61028&REV_C1  ; DJ2_MV
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_049E1028&REV_C1  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_049F1028&REV_C1  ; DJ2_CP_UMA
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04A01028&REV_C1  ; DJ2_CP_DIS
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04DF1028&REV_C1  ; Andros MLK

%Atheros.L2cb%  =       L2cb.ShutOn.ndi,            PCI\VEN_1969&DEV_2060&SUBSYS_147E103C&REV_C1  ; Bixby 3.0

%Atheros.L2cb%  =       L2cb.ShutOn.ndi,            PCI\VEN_1969&DEV_2060&SUBSYS_FD501179&REV_C1  ; TE2
%Atheros.L2cb%  =       L2cb.ShutOn.ndi,            PCI\VEN_1969&DEV_2060&SUBSYS_FDD01179&REV_C1  ; BL6

%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_04291025&REV_C1  ; ZH9
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_043D1025&REV_C1  ; ZH9
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_043E1025&REV_C1  ; ZH9AB
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_03491025&REV_C1  ; NAV70
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_034A1025&REV_C1  ; NAV80
%Atheros.L2cb%  =       L2cb.ASPM1.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_04971025&REV_C1  ; PAV50
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_048A1025&REV_C1  ; PEW72
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_05431025&REV_C1  ; P0VE6
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_05441025&REV_C1  ; P0VS6

%Atheros.L2cb%  =       L2cb.DisS5.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_396517AA&REV_C1  ; LL7
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_396B17AA&REV_C1  ; NAWEx
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_397917AA&REV_C1  ; PIWG1/2/3
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_397B17AA&REV_C1  ; PAWGx
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_398317AA&REV_C1  ; PAW10/20

%Atheros.L2cb%  =       L2cb.ECS.ndi,               PCI\VEN_1969&DEV_2060&SUBSYS_81521019&REV_C1  ; ECS

%Atheros.L2cb%  =       L2cb.FUJU.ndi,              PCI\VEN_1969&DEV_2060&SUBSYS_15DB10CF&REV_C1  ; UME

%Atheros.L2cb%  =       L2cb.DisS5.ndi,             PCI\VEN_1969&DEV_2060&SUBSYS_18501043&REV_C1  ; ASUS
%Atheros.L2cb%  =       L2cb.ndi,                   PCI\VEN_1969&DEV_2060&SUBSYS_84681043&REV_C1  ; ASUS

%Atheros.L2cb%  =       L2cb.ECS.ndi,               PCI\VEN_1969&DEV_2060&SUBSYS_E0001458&REV_C1  ; GIGABYTE

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073		          ; L1d
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_10731969&REV_C0  ; L1d

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03561025&REV_C0  ; ZQ1
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03571025&REV_C0  ; ZQ1
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03581025&REV_C0  ; ZQ1B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03591025&REV_C0  ; ZQ1B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_035A1025&REV_C0  ; ZR7
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_035B1025&REV_C0  ; ZR7
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_035C1025&REV_C0  ; ZR7B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_035D1025&REV_C0  ; ZR7B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_035E1025&REV_C0  ; ZQ2
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03601025&REV_C0  ; ZR8
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03621025&REV_C0  ; ZR8B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03661025&REV_C0  ; ZQ2B
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03641025&REV_C0  ; JM31
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03671025&REV_C0  ; ZYA
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_03681025&REV_C0  ; ZYA
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_038B1025&REV_C0  ; ZYB
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_038C1025&REV_C0  ; ZYB
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04121025&REV_C0  ; ZYD
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_040E1025&REV_C0  ; JV10
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04281025&REV_C0  ; SJV10
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04291025&REV_C0  ; JV10_NL
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_040D1025&REV_C0  ; SJV10_NL
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04601025&REV_C0  ; JV10_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_045F1025&REV_C0  ; JV10_NL
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04631025&REV_C0  ; ZR7D
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04641025&REV_C0  ; JV53_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04651025&REV_C0  ; JV53_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04731025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04751025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04761025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_047E1025&REV_C0  ; PAU30
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_048A1025&REV_C0  ; PEW72
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_050E1025&REV_C0  ; P7YE0
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_050F1025&REV_C0  ; P7YE0
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_05131025&REV_C0  ; P7YS0
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_05141025&REV_C0  ; P7YS0
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_05151025&REV_C0  ; P7YH0
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_05161025&REV_C0  ; P7YH0
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_054C1025&REV_C0  ; JM30
%Atheros.L1d%  =        L1d.TxPerf.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_054E1025&REV_C0  ; JM30
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_05221025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_05231025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_05241025&REV_C0  ; SJ53
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_052A1025&REV_C0  ; SJ53
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_05571025&REV_C0  ; JE41
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_055F1025&REV_C0  ; JE51
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_054B1025&REV_C0  ; HM51
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_054D1025&REV_C0  ; HM51
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_054F1025&REV_C0  ; JE40
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_055B1025&REV_C0  ; JE50
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_05711025&REV_C0  ; SJM40
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_056D1025&REV_C0  ; BA70
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_056F1025&REV_C0  ; SJM50

%Atheros.L1d%  =        L1d.ShutOn.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_FD501179&REV_C0  ; TE2
%Atheros.L1d%  =        L1d.ShutOn.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_FDD01179&REV_C0  ; BL6
%Atheros.L1d%  =        L1d.ToPatch.ndi,            PCI\VEN_1969&DEV_1073&SUBSYS_FF1E1179&REV_C0  ; Berlin

%Atheros.L1d%  =        L1d.DisS5.ndi,              PCI\VEN_1969&DEV_1073&SUBSYS_395B17AA&REV_C0  ; NAU00
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_396A17AA&REV_C0  ; NAWEx
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_395817AA&REV_C0  ; NIUM1
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_397917AA&REV_C0  ; PIWG1/2/3
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_397B17AA&REV_C0  ; PAWGx
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_398317AA&REV_C0  ; PAW10/20

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_0CDD105B&REV_C0  ; W930
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_0D5E105B&REV_C0  ; Haier
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_0DBE105B&REV_C0  ; Clone

%Atheros.L1d%  =        L1d.ECS.ndi,                PCI\VEN_1969&DEV_1073&SUBSYS_81511019&REV_C0  ; ECS
%Atheros.L1d%  =        L1d.ECSD.ndi,               PCI\VEN_1969&DEV_1073&SUBSYS_04731028&REV_C0  ; ECS/Dell

%Atheros.L1d%  =        L1d.DisS5.ndi,              PCI\VEN_1969&DEV_1073&SUBSYS_18041043&REV_C0  ; ASUS
%Atheros.L1d%  =        L1d.DisS5.ndi,              PCI\VEN_1969&DEV_1073&SUBSYS_18401043&REV_C0  ; ASUS

%Atheros.L1d%  =        L1d.GIGABYTE.ndi,           PCI\VEN_1969&DEV_1073&SUBSYS_E0001458&REV_C0  ; GIGABYTE

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08611854&REV_C0  ; QLH
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08621854&REV_C0  ; QLH
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08631854&REV_C0  ; QLH        
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08641854&REV_C0  ; QLH       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08651854&REV_C0  ; QLH       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08661854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08671854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08681854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08691854&REV_C0  ; QLC       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08701854&REV_C0  ; QLC       
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_08711854&REV_C0  ; QLC

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04511028&REV_C0  ; DJ1_MV
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04661028&REV_C0  ; DJ1_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_046F1028&REV_C0  ; DJ1_AMD
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04861028&REV_C0  ; DJ2_CP
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04871028&REV_C0  ; DJ2_AMD
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_048F1028&REV_C0  ; Dell_Avenger
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04901028&REV_C0  ; Dell_Voyager
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04A61028&REV_C0  ; DJ2_MV
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_049E1028&REV_C0  ; DJ2_AMD
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_049F1028&REV_C0  ; DJ2_CP_UMA
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04A01028&REV_C0  ; DJ2_CP_DIS
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04911028&REV_C0  ; Spector
%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_04C81028&REV_C0  ; Alienware

%Atheros.L1d%  =        L1d.ndi,                    PCI\VEN_1969&DEV_1073&SUBSYS_2AAE103C&REV_C0  ; Pegatron
%Atheros.L1d%  =        L1d.ShutOn.ndi,             PCI\VEN_1969&DEV_1073&SUBSYS_207D1B0A&REV_C0  ; Pegatron

%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062                         ; L2cb 2.0
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_20621969&REV_C0  ; L2cb 2.0

%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04861028&REV_C0  ; DJ2_CP
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04871028&REV_C0  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04511028&REV_C0  ; DJ1_MV
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04551028&REV_C0  ; UM7
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04561028&REV_C0  ; UM8
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04571028&REV_C0  ; UM9
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04661028&REV_C0  ; DJ1_CP
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_046F1028&REV_C0  ; DJ1_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_048F1028&REV_C0  ; Dell_Avenger
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04901028&REV_C0  ; Dell_Voyager
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04A61028&REV_C0  ; DJ2_MV
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_049E1028&REV_C0  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_049F1028&REV_C0  ; DJ2_CP_UMA
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04A01028&REV_C0  ; DJ2_CP_DIS

%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FF1E1179&REV_C0  ; IEC

%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_147E103C&REV_C0  ; Bixby 3.0

%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD501179&REV_C0  ; TE2
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FDD01179&REV_C0  ; BL6

%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C0  ; ZH9
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_043D1025&REV_C0  ; ZH9
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_043E1025&REV_C0  ; ZH9AB
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_03491025&REV_C0  ; NAV70
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_034A1025&REV_C0  ; NAV80
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04971025&REV_C0  ; PAV50
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_048A1025&REV_C0  ; PEW72
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_02291025&REV_C0  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_027F1025&REV_C0  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_02801025&REV_C0  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_03641025&REV_C0  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_040E1025&REV_C0  ; JV10
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04281025&REV_C0  ; SJV10
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C0  ; JV10_NL
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_040D1025&REV_C0  ; SJV10_NL
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04601025&REV_C0  ; SJV10_CP
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_045F1025&REV_C0  ; JV10_NL

%Atheros.L2cb%  =       L2cb2.DisS5.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_396517AA&REV_C0  ; LL7
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_396B17AA&REV_C0  ; NAWEx
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_397917AA&REV_C0  ; PIWG1/2/3
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_397B17AA&REV_C0  ; PAWGx
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_398317AA&REV_C0  ; PAW10/20

%Atheros.L2cb%  =       L2cb2.ECS.ndi,              PCI\VEN_1969&DEV_2062&SUBSYS_81521019&REV_C0  ; ECS

%Atheros.L2cb%  =       L2cb2.FUJU.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_15DB10CF&REV_C0  ; UME

%Atheros.L2cb%  =       L2cb2.DisS5.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_18501043&REV_C0  ; ASUS
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_84681043&REV_C0  ; ASUS

%Atheros.L2cb%   =      L2cb2.GIGABYTE.ndi,         PCI\VEN_1969&DEV_2062&SUBSYS_E0001458&REV_C0  ; GIGABYTE

%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_20621969&REV_C1  ; L2cb 2.1

%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04861028&REV_C1  ; DJ2_CP
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04871028&REV_C1  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04511028&REV_C1  ; DJ1_MV
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04551028&REV_C1  ; UM7
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04561028&REV_C1  ; UM8
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04571028&REV_C1  ; UM9
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04661028&REV_C1  ; DJ1_CP
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_046F1028&REV_C1  ; DJ1_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_048F1028&REV_C1  ; Dell_Avenger
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04901028&REV_C1  ; Dell_Voyager
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04A61028&REV_C1  ; DJ2_MV
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_049E1028&REV_C1  ; DJ2_AMD
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_049F1028&REV_C1  ; DJ2_CP_UMA
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04A01028&REV_C1  ; DJ2_CP_DIS
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04DF1028&REV_C1  ; Andros MLK
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04EA1028&REV_C1  ; Zuma
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_051B1028&REV_C1  ; Shakira

%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FC761179&REV_C1  ; Ankara
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FC771179&REV_C1  ; Ankara
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD7A1179&REV_C1  ; Ankara
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD7B1179&REV_C1  ; Ankara
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FC671179&REV_C1  ; Celtic
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD6A1179&REV_C1  ; Celtic
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD6B1179&REV_C1  ; Celtic
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD501179&REV_C1  ; TE2
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FDD01179&REV_C1  ; BL6
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FF1E1179&REV_C1  ; IEC
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FDD11179&REV_C1  ; TE7
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FFD61179&REV_C1  ; TZ6
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FCB31179&REV_C1  ; TE7
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FC501179&REV_C1  ; BLF
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FCD01179&REV_C1  ; TE5
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FCC01179&REV_C1  ; BU5
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD521179&REV_C1  ; BLE
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FDD21179&REV_C1  ; BU4
%Atheros.L2cb%  =       L2cb2.PWMAll.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_FD401179&REV_C1  ; BU4

%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_147E103C&REV_C1  ; Bixby 3.0
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_3584103C&REV_C1  ; Kitty
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_3585103C&REV_C1  ; Kitty
%Atheros.L2cb%  =       L2cb2.ShutOn.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_3595103C&REV_C1  ; KID

%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C1  ; ZH9
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_043D1025&REV_C1  ; ZH9
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_043E1025&REV_C1  ; ZH9AB
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_03491025&REV_C1  ; NAV70
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_034A1025&REV_C1  ; NAV80
%Atheros.L2cb%  =       L2cb2.ASPM1.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_04971025&REV_C1  ; PAV50
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_048A1025&REV_C1  ; PEW72
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_02291025&REV_C1  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_027F1025&REV_C1  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_02801025&REV_C1  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_03641025&REV_C1  ; JM31
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_040E1025&REV_C1  ; JV10
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04281025&REV_C1  ; SJV10
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04291025&REV_C1  ; JV10_NL
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_040D1025&REV_C1  ; SJV10_NL
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_04601025&REV_C1  ; SJV10_CP
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_045F1025&REV_C1  ; JV10_NL
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_05431025&REV_C1  ; P0VE6
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_05441025&REV_C1  ; P0VS6
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_05981025&REV_C1  ; P1VE6
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06021025&REV_C1  ; HMA51-BZ
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06031025&REV_C1  ; ZQJ
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06041025&REV_C1  ; ZQQ
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_060A1025&REV_C1  ; SAZ70
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_060B1025&REV_C1  ; SIC70
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_060E1025&REV_C1  ; SAZ71
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_060F1025&REV_C1  ; SIC71
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06101025&REV_C1  ; AIC70
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06111025&REV_C1  ; AIC71
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06141025&REV_C1  ; AAB70
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06151025&REV_C1  ; AAB71
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_05041025&REV_C1  ;
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_061E1025&REV_C1  ; Q5WP1
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06221025&REV_C1  ; HMA41
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_06231025&REV_C1  ; HMA51

%Atheros.L2cb%  =       L2cb2.DisS5.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_396517AA&REV_C1  ; LL7
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_396B17AA&REV_C1  ; NAWEx
%Atheros.L2cb%  =       L2cb2.TxPerf.ndi,           PCI\VEN_1969&DEV_2062&SUBSYS_397917AA&REV_C1  ; PIWG1/2/3
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_397B17AA&REV_C1  ; PAWGx
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_398317AA&REV_C1  ; PAW10/20

%Atheros.L2cb%  =       L2cb2.ECS.ndi,              PCI\VEN_1969&DEV_2062&SUBSYS_81521019&REV_C1  ; ECS

%Atheros.L2cb%  =       L2cb2.FUJU.ndi,             PCI\VEN_1969&DEV_2062&SUBSYS_15DB10CF&REV_C1  ; UME

%Atheros.L2cb%  =       L2cb2.DisS5.ndi,            PCI\VEN_1969&DEV_2062&SUBSYS_18501043&REV_C1  ; ASUS
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_84681043&REV_C1  ; ASUS
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_100B1043&REV_C1  ; ASUS

%Atheros.L2cb%   =      L2cb2.GIGABYTE.ndi,         PCI\VEN_1969&DEV_2062&SUBSYS_E0001458&REV_C1  ; GIGABYTE

%Atheros.L2cb%   =      L2cb2.GIGABYTE.ndi,         PCI\VEN_1969&DEV_2062&SUBSYS_28021565&REV_C1  ; BIOSTAR
%Atheros.L2cb%   =      L2cb2.GIGABYTE.ndi,         PCI\VEN_1969&DEV_2062&SUBSYS_28011565&REV_C1  ; BIOSTAR

%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_207E1B0A&REV_C1  ; Pegatron
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_2AAE103C&REV_C1  ; Pegatron
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_3580103C&REV_C1  ; Pegatron
%Atheros.L2cb%  =       L2cb2.ndi,                  PCI\VEN_1969&DEV_2062&SUBSYS_2AD1103C&REV_C1  ; Pegatron

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083		          ; L1d v2.0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_10831969&REV_C0  ; L1d

%Atheros.L1d%  =        L1d2.DisS5.ndi,             PCI\VEN_1969&DEV_1083&SUBSYS_18401043&REV_C0  ; ASUS
%Atheros.L1d%  =        L1d2.DisS5.ndi,             PCI\VEN_1969&DEV_1083&SUBSYS_18511043&REV_C0  ; ASUS
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_847E1043&REV_C0  ; ASUS
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_84BF1043&REV_C0  ; ASUS
%Atheros.L1cd%  =       L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_83FE1043&REV_C0  ; ASUS

%Atheros.L1d%  =        L1d2.GIGABYTE.ndi,          PCI\VEN_1969&DEV_1083&SUBSYS_E0001458&REV_C0  ; GIGABYTE

%Atheros.L1d%  =        L1d2.ECS.ndi,               PCI\VEN_1969&DEV_1083&SUBSYS_81511019&REV_C0  ; ECS

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_2AAE103C&REV_C0  ; Pegatron
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_3580103C&REV_C0  ; Pegatron
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_109C1462&REV_C0  ; Pegatron
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_208D1B0A&REV_C0  ; Pegatron

%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3584103C&REV_C0  ; Kitty
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3585103C&REV_C0  ; Kitty
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3385103C&REV_C0  ; UMA
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3386103C&REV_C0  ; DIS
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_1688103C&REV_C0  ; Lauren
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_1689103C&REV_C0  ; Vuitton
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_168A103C&REV_C0  ; Vuitton

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04631025&REV_C0  ; ZR7D
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_047E1025&REV_C0  ; PAU30
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_048A1025&REV_C0  ; PEW72
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_050E1025&REV_C0  ; P7YE0
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_050F1025&REV_C0  ; P7YE0
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_05131025&REV_C0  ; P7YS0
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_05141025&REV_C0  ; P7YS0
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_05151025&REV_C0  ; P7YH0
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_05161025&REV_C0  ; P7YH0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_054C1025&REV_C0  ; JM30
%Atheros.L1d%  =        L1d2.TxPerf.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_054E1025&REV_C0  ; JM30
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_02291025&REV_C0  ; JM31
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_027F1025&REV_C0  ; JM31
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_02801025&REV_C0  ; JM31
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03641025&REV_C0  ; JM31
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_040E1025&REV_C0  ; JV10
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04281025&REV_C0  ; SJV10
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04291025&REV_C0  ; JV10_NL
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_040D1025&REV_C0  ; SJV10_NL
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04601025&REV_C0  ; SJV10_CP
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_045F1025&REV_C0  ; JV10_NL
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03561025&REV_C0  ; ZQ1
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03571025&REV_C0  ; ZQ1
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03581025&REV_C0  ; ZQ1B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03591025&REV_C0  ; ZQ1B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_035A1025&REV_C0  ; ZR7
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_035B1025&REV_C0  ; ZR7
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_035C1025&REV_C0  ; ZR7B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_035D1025&REV_C0  ; ZR7B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_035E1025&REV_C0  ; ZQ2
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03601025&REV_C0  ; ZR8
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03621025&REV_C0  ; ZR8B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03661025&REV_C0  ; ZQ2B
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03641025&REV_C0  ; JM31
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03671025&REV_C0  ; ZYA
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_03681025&REV_C0  ; ZYA
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_038B1025&REV_C0  ; ZYB
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_038C1025&REV_C0  ; ZYB
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04121025&REV_C0  ; ZYD
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_040E1025&REV_C0  ; JV10
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04281025&REV_C0  ; SJV10
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04291025&REV_C0  ; JV10_NL
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_040D1025&REV_C0  ; SJV10_NL
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04601025&REV_C0  ; JV10_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_045F1025&REV_C0  ; JV10_NL
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04631025&REV_C0  ; ZR7D
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04641025&REV_C0  ; JV53_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04651025&REV_C0  ; JV53_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04731025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04751025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04761025&REV_C0  ; SJM70_CP
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_048A1025&REV_C0  ; PEW72
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_051E1025&REV_C0  ; SJV73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_051F1025&REV_C0  ; SJV73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05201025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05211025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05221025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05231025&REV_C0  ; JE73
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05241025&REV_C0  ; SJ53
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_052A1025&REV_C0  ; SJ53
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_052D1025&REV_C0  ; ZQE
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_052E1025&REV_C0  ; ZQE
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_052F1025&REV_C0  ; ZQG
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05301025&REV_C0  ; ZQG
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05571025&REV_C0  ; JE41
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_055F1025&REV_C0  ; JE51
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_054B1025&REV_C0  ; HM51
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_054D1025&REV_C0  ; HM51
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_054F1025&REV_C0  ; JE40
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_055B1025&REV_C0  ; JE50
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05711025&REV_C0  ; SJM40
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_056D1025&REV_C0  ; BA70
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_056F1025&REV_C0  ; SJM50
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05731025&REV_C0  ; ZRJ
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05741025&REV_C0  ; ZRJ
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_058D1025&REV_C0  ; SJV51
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_058E1025&REV_C0  ; SJV51
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_059C1025&REV_C0  ; JE70
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_059D1025&REV_C0  ; SJV70
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_059C1025&REV_C0  ; JE70
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_059D1025&REV_C0  ; SJV70
%Atheros.L1d%  =        L1d2.Pega.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_05391025&REV_C0  ; EIH30
%Atheros.L1d%  =        L1d2.Pega.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_053A1025&REV_C0  ; EIH31
%Atheros.L1d%  =        L1d2.Pega.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_060C1025&REV_C0  ; EIH30A
%Atheros.L1d%  =        L1d2.Pega.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_060D1025&REV_C0  ; EIH31A

%Atheros.L1d%  =        L1D2.WOLNone.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_048F1028&REV_C0  ; Dell_Avenger
%Atheros.L1d%  =        L1D2.WOLNone.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_04901028&REV_C0  ; Dell_Voyager
%Atheros.L1d%  =        L1D2.WOLNone.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_04911028&REV_C0  ; Spector
%Atheros.L1d%  =        L1D2.WOLNone.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_04C81028&REV_C0  ; Alienware
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04A61028&REV_C0  ; DJ2_MV
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_049E1028&REV_C0  ; DJ2_AMD
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_049F1028&REV_C0  ; DJ2_CP_UMA
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04A01028&REV_C0  ; DJ2_CP_DIS
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04371028&REV_C0  ; Miso
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04461028&REV_C0  ; Panerai
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_04841028&REV_C0  ; UMA
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_051F1028&REV_C0  ; UMA1
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05201028&REV_C0  ; UMA2
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05211028&REV_C0  ; UMA3
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05221028&REV_C0  ; Discrete1
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05231028&REV_C0  ; Discrete2
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_05241028&REV_C0  ; Discrete3

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_397917AA&REV_C0  ; PIWG1/2/3
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_397B17AA&REV_C0  ; PAWGx
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_398317AA&REV_C0  ; PAW10/20
%Atheros.L1d%  =        L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21EC17AA&REV_C0  ; Davis
%Atheros.L1d%  =        L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21ED17AA&REV_C0  ; Davis
%Atheros.L1d%  =        L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21EE17AA&REV_C0  ; Payton
%Atheros.L1d%  =        L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21EF17AA&REV_C0  ; Payton
%Atheros.L1d%  =        L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21F017AA&REV_C0  ; Payton
%Atheros.L1d%  =       	L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21F117AA&REV_C0  ; Payton
%Atheros.L1d%  =       	L1d2.LVOn.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_21F217AA&REV_C0  ; Payton

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08611854&REV_C0  ; QLH
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08621854&REV_C0  ; QLH
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08631854&REV_C0  ; QLH        
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08641854&REV_C0  ; QLH       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08651854&REV_C0  ; QLH       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08661854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08671854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08681854&REV_C0  ; QLA       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08691854&REV_C0  ; QLC       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08701854&REV_C0  ; QLC       
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08711854&REV_C0  ; QLC
%Atheros.L1d%  =       	L1d2.ndi,              	    PCI\VEN_1969&DEV_1083&SUBSYS_08891854&REV_C0  ; QLM
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08901854&REV_C0  ; QLM
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08911854&REV_C0  ; QLM
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08921854&REV_C0  ; QLM
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08961854&REV_C0  ; LG2
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08971854&REV_C0  ; LG2
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08981854&REV_C0  ; LG2
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_08991854&REV_C0  ; LG4
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09001854&REV_C0  ; LG4
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09011854&REV_C0  ; LG4
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09021854&REV_C0  ; LG7
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09031854&REV_C0  ; LG7
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09041854&REV_C0  ; LG7    
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09061854&REV_C0  ; A430
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09071854&REV_C0  ; A430
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_09081854&REV_C0  ; A430
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_17911854&REV_C0  ; A420
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_17921854&REV_C0  ; A430
%Atheros.L1d%  =       	L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_17931854&REV_C0  ; A430   

%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_1650103C&REV_C0  ; Zidane UMA
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_1651103C&REV_C0  ; Zidane SG
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3595103C&REV_C0  ; KID
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_3596103C&REV_C0  ; KID

%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FDD11179&REV_C0  ; TE7
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FFD61179&REV_C0  ; TZ6
%Atheros.L1d%  =        L1d2.Toshiba.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_FF1E1179&REV_C0  ; WS2
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FCB01179&REV_C0  ; TZ6
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FC501179&REV_C0  ; BLF
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FCD01179&REV_C0  ; TE5
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FCC01179&REV_C0  ; BU5
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FD521179&REV_C0  ; BLE
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FDD21179&REV_C0  ; BU4
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FD401179&REV_C0  ; BU4
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FDD01179&REV_C0  ; TE4
%Atheros.L1d%  =        L1d2.PWMAll.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FD501179&REV_C0  ; BLG
%Atheros.L1d%  =        L1d2.ShutOn.ndi,            PCI\VEN_1969&DEV_1083&SUBSYS_FC661179&REV_C0  ; Celtic

%Atheros.L1d%  =        L1d2.SONY.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_9080104D&REV_C0  ; V050
%Atheros.L1d%  =        L1d2.SONY.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_9081104D&REV_C0  ; V050
%Atheros.L1d%  =        L1d2.WOLNone.ndi,           PCI\VEN_1969&DEV_1083&SUBSYS_908A104D&REV_C0  ; Z40/50
%Atheros.L1d%  =        L1d2.SONY.ndi,              PCI\VEN_1969&DEV_1083&SUBSYS_908D104D&REV_C0  ; Z40/50BR

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0872152D&REV_C0  ; LG
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0873152D&REV_C0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0875152D&REV_C0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0876152D&REV_C0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0877152D&REV_C0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0878152D&REV_C0
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0883152D&REV_C0  ; SW6H
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0884152D&REV_C0  ; SW6H
%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0880152D&REV_C0  ; SWH

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_10E717C0&REV_C0  ; M51

%Atheros.L1d%  =        L1d2.ndi,                   PCI\VEN_1969&DEV_1083&SUBSYS_0DBE105B&REV_C0  ; Clone

%Atheros.L1d%  =        L1d2.ECS.ndi,               PCI\VEN_1969&DEV_1083&SUBSYS_28031565&REV_C0  ; BIOSTAR

; Windows NT specific entry
[L1c.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1c.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1c.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1c.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.Toshiba.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, Toshiba.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1c.Toshiba.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.GIGABYTE.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L1c.GIGABYTE.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.SONY.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLNone.params
CopyFiles       = L1c.CopyFiles

[L1c.SONY.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1c.WOLMagic.ndi]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L1c.WOLMagic.ndi.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2c.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2c.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2c.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.Toshiba.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, Toshiba.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2c.Toshiba.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.GIGABYTE.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L2c.GIGABYTE.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.SONY.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLNone.params
CopyFiles       = L1c.CopyFiles

[L2c.SONY.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.WOLMagic.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L2c.WOLMagic.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L2c.ECS.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.FUJU.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, FUJU.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2c.FUJU.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.PWMAll.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params
CopyFiles       = L1c.CopyFiles

[L2c.PWMAll.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2c.ASPM1.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, ASPM1M.params
CopyFiles       = L1c.CopyFiles

[L2c.ASPM1.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2cb.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2cb.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.PWMAll.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params
CopyFiles       = L1c.CopyFiles

[L2cb.PWMAll.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2cb.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L2cb.ECS.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.FUJU.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, FUJU.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L2cb.FUJU.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb.ASPM1.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L2cb.Params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, ASPM1M.params
CopyFiles       = L1c.CopyFiles

[L2cb.ASPM1.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.TxPerf.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L2cb2.TxPerf.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.Toshiba.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, Toshiba.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.Toshiba.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.GIGABYTE.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.GIGABYTE.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.SONY.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLNone.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.SONY.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.WOLMagic.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.WOLMagic.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.ECS.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.FUJU.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, FUJU.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.FUJU.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.PWMAll.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.PWMAll.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L2cb2.ASPM1.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, ASPM1M.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L2cb2.ASPM1.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1d.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.TxPerf.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d.TxPerf.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1d.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.ToPatch.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params, ToPatch.params
CopyFiles       = L1c.CopyFiles

[L1d.ToPatch.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.PWMAll.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params
CopyFiles       = L1c.CopyFiles

[L1d.PWMAll.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, WOLDefault.params
CopyFiles       = L1c.CopyFiles

[L1d.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.GIGABYTE.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, LongCable.params
CopyFiles       = L1c.CopyFiles

[L1d.GIGABYTE.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L1d.ECS.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d.ECSD.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, ECS.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params
CopyFiles       = L1c.CopyFiles

[L1d.ECSD.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.WOLNone.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLNone.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.WOLNone.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.TxPerf.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d2.TxPerf.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.ShutOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d2.ShutOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.LVOn.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, ECS.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params, Toshiba.params
CopyFiles       = L1c.CopyFiles

[L1d2.LVOn.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.LV.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, ECS.Params, Common.Params.WinNT, ShutOff.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d2.LV.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.PWMAll.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.PWMAll.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.DisS5.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, WOLDefault.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.DisS5.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.GIGABYTE.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, EEELPI.params, LongCable.params
CopyFiles       = L1c.CopyFiles

[L1d2.GIGABYTE.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.ECS.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.ECS.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.ECSD.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, ECS.Params, Common.Params.WinNT, ShutOn.params, WOLMagic.params, EEELPI.params
CopyFiles       = L1c.CopyFiles

[L1d2.ECSD.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.SONY.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Common.Params.WinNT, WOLDefault.params, EEELPIEn.params
CopyFiles       = L1c.CopyFiles

[L1d2.SONY.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.Toshiba.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.Params, Common.Params, Common.Params.WinNT, ShutOn.params, WOLDefault.params, PWMAll.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d2.Toshiba.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog

[L1d2.Pega.ndi.NT]
Characteristics = 0x84
BusType         = 5              ;PCI
AddReg          = L1c.reg, L1c.params, Common.Params, Pega.Params.WinNT, ShutOn.params, WOLDefault.params, EEELPI.params, TxPerf.params
CopyFiles       = L1c.CopyFiles

[L1d2.Pega.ndi.NT.Services]
AddService = L1c, 2, L1c.Service, Common.EventLog
;-----------------------------------------------------------------------------
; L1c NT specific
;
[L1c.reg]
HKR, Ndi, HelpText,, %HelpText%
HKR, Ndi, Service,    0, "L1c"
; use ndis5 as the upper bound because NT supports it
HKR, Ndi\Interfaces, UpperRange, 0, "ndis5"
HKR, Ndi\Interfaces, LowerRange, 0, "ethernet"

[L1c.Service]
DisplayName     = %L1c.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\l1c51x86.sys
LoadOrderGroup  = NDIS

[common.EventLog]
AddReg = common.AddEventLog.reg

[common.AddEventLog.reg]
HKR,, EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\Drivers\l1c51x86.sys"
HKR,, TypesSupported,   0x00010001, 7

[Toshiba.params]
HKR,, WOLMode,	        0x00010001, 1

[ToPatch.params]
HKR,, ToPatch,          0x00010001, 1

[PWMNone.params]
HKR,, PnPCapabilities,	0x00010001, 0x0038

[PWM.params]
HKR,, PnPCapabilities,	0x00010001, 0x0020

[PWMAll.params]
HKR,, PnPCapabilities,	0x00010001, 0x0120

[ASPM1M.params]
HKR,, ASPMLim,	        0x00010001, 1

[ASPM10M.params]
HKR,, ASPMLim,	        0x00010001, 2

[ASPM100M.params]
HKR,, ASPMLim,	        0x00010001, 3

[LongCable.params]
HKR,, LongCable,        0x00010001, 1

[TxPerf.params]
HKR,, TxPerf,           0x00010001, 1

[L1c.params]
HKR,Ndi\params\JumboPacket,        		ParamDesc,  0, 		%JumboFrame%
HKR,Ndi\params\JumboPacket,        		Default,    0, 		"1514"
HKR,Ndi\params\JumboPacket,        		Type,       0, 		"enum"
HKR,Ndi\params\JumboPacket\enum,   		"1514",     0, 		%Off%
HKR,Ndi\params\JumboPacket\enum,   		"2048",     0, 		%2KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"3072",     0, 		%3KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"4096",     0, 		%4KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"5120",     0, 		%5KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"6144",     0, 		%6KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"7168",     0, 		%7KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"8192",     0, 		%8KBMTU%
HKR,Ndi\params\JumboPacket\enum,   		"9216",     0, 		%9KBMTU%

[L2cb.Params]
HKR, Ndi\Params\APSmode,    	                ParamDesc,  0,          %APSmode%
HKR, Ndi\Params\APSmode,    	                Type,       0,          "enum"
HKR, Ndi\Params\APSmode,    	                Default,    0,          "0"
HKR, Ndi\Params\APSmode\enum, 	                "1",        0,          %On%
HKR, Ndi\Params\APSmode\enum, 	                "0",        0,          %Off%

[Common.Params]
HKR, Ndi\Params\NetworkAddress, 		ParamDesc,  0, 		%NetAddr%
HKR, Ndi\Params\NetworkAddress, 		Type,       0,      	"edit"
HKR, Ndi\Params\NetworkAddress, 		LimitText,  0, 		"18"
HKR, Ndi\Params\NetworkAddress, 		UpperCase,  0, 		"1"
HKR, Ndi\Params\NetworkAddress, 		Default,    0,   	""
HKR, Ndi\Params\NetworkAddress, 		Optional,   0,  	"1"

HKR, Ndi\Params\MaxInterrupt,   		ParamDesc,  0, 		%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,   		Type,       0,      	"int"
HKR, Ndi\Params\MaxInterrupt,   		Base,       0,      	"10"
HKR, Ndi\Params\MaxInterrupt,   		Min,        0,       	"1000"
HKR, Ndi\Params\MaxInterrupt,   		Max,        0,       	"30000"
HKR, Ndi\Params\MaxInterrupt,   		Step,       0,      	"200"
HKR, Ndi\Params\MaxInterrupt,   		Default,    0,   	"5000"

HKR, Ndi\Params\MediaType,  			ParamDesc,  0,     	%MediaType%
HKR, Ndi\Params\MediaType,  			Type,       0,          "enum"
HKR, Ndi\Params\MediaType,  			Default,    0,       	"0"
HKR, Ndi\Params\MediaType\enum,     		"0",        0,   	%Auto%
HKR, Ndi\Params\MediaType\enum,     		"1",        0,   	%100MFD%
HKR, Ndi\Params\MediaType\enum,     		"2",        0,   	%100MHD%
HKR, Ndi\Params\MediaType\enum,     		"3",        0,   	%10MFD%
HKR, Ndi\Params\MediaType\enum,     		"4",        0,   	%10MHD%

HKR, Ndi\Params\FlowControl,    		ParamDesc,  0,  	%FlowCtrl%
HKR, Ndi\Params\FlowControl,    		Type,       0,       	"enum"
HKR, Ndi\Params\FlowControl,    		Default,    0,    	"1"
HKR, Ndi\Params\FlowControl\enum, 		"1",        0,      	%On%
HKR, Ndi\Params\FlowControl\enum, 		"0",        0,      	%Off%

HKR, Ndi\Params\VLanID,				ParamDesc,  0,          %VLanID%
HKR, Ndi\Params\VLanID,   		        Base,       0,      	"10"
HKR, Ndi\Params\VLanID,				Type,	    0,          "long"
HKR, Ndi\Params\VLanID,				Min,        0,          "0"
HKR, Ndi\Params\VLanID,				Max,        0,          "4094"
HKR, Ndi\Params\VLanID,				Step,       0,          "1"
HKR, Ndi\Params\VLanID,				Default,    0,          "0"

[FUJU.Params]
HKR, Ndi\Params\NetworkAddress, 		ParamDesc,  0, 		%NetAddr%
HKR, Ndi\Params\NetworkAddress, 		Type,       0,      	"edit"
HKR, Ndi\Params\NetworkAddress, 		LimitText,  0, 		"18"
HKR, Ndi\Params\NetworkAddress, 		UpperCase,  0, 		"1"
HKR, Ndi\Params\NetworkAddress, 		Default,    0,   	""
HKR, Ndi\Params\NetworkAddress, 		Optional,   0,  	"1"

HKR, Ndi\Params\MaxInterrupt,   		ParamDesc,  0, 		%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,   		Type,       0,      	"int"
HKR, Ndi\Params\MaxInterrupt,   		Base,       0,      	"10"
HKR, Ndi\Params\MaxInterrupt,   		Min,        0,       	"1000"
HKR, Ndi\Params\MaxInterrupt,   		Max,        0,       	"30000"
HKR, Ndi\Params\MaxInterrupt,   		Step,       0,      	"200"
HKR, Ndi\Params\MaxInterrupt,   		Default,    0,   	"5000"

HKR, Ndi\Params\MediaType,  			ParamDesc,  0,     	%MediaType%
HKR, Ndi\Params\MediaType,  			Type,       0,          "enum"
HKR, Ndi\Params\MediaType,  			Default,    0,       	"0"
HKR, Ndi\Params\MediaType\enum,     		"0",        0,   	%Auto%
HKR, Ndi\Params\MediaType\enum,     		"1",        0,   	%100MFD%
HKR, Ndi\Params\MediaType\enum,     		"2",        0,   	%100MHD%
HKR, Ndi\Params\MediaType\enum,     		"3",        0,   	%10MFD%
HKR, Ndi\Params\MediaType\enum,     		"4",        0,   	%10MHD%

HKR, Ndi\Params\FlowControl,    		ParamDesc,  0,  	%FlowCtrl%
HKR, Ndi\Params\FlowControl,    		Type,       0,       	"enum"
HKR, Ndi\Params\FlowControl,    		Default,    0,    	"0"
HKR, Ndi\Params\FlowControl\enum, 		"1",        0,      	%On%
HKR, Ndi\Params\FlowControl\enum, 		"0",        0,      	%Off%

HKR, Ndi\Params\VLanID,				ParamDesc,  0,          %VLanID%
HKR, Ndi\Params\VLanID,   		        Base,       0,      	"10"
HKR, Ndi\Params\VLanID,				Type,	    0,          "long"
HKR, Ndi\Params\VLanID,				Min,        0,          "0"
HKR, Ndi\Params\VLanID,				Max,        0,          "4094"
HKR, Ndi\Params\VLanID,				Step,       0,          "1"
HKR, Ndi\Params\VLanID,				Default,    0,          "0"

[ECS.Params]
HKR, Ndi\Params\NetworkAddress, 		ParamDesc,  0, 		%NetAddr%
HKR, Ndi\Params\NetworkAddress, 		Type,       0,      	"edit"
HKR, Ndi\Params\NetworkAddress, 		LimitText,  0, 		"18"
HKR, Ndi\Params\NetworkAddress, 		UpperCase,  0, 		"1"
HKR, Ndi\Params\NetworkAddress, 		Default,    0,   	""
HKR, Ndi\Params\NetworkAddress, 		Optional,   0,  	"1"

HKR, Ndi\Params\MaxInterrupt,   		ParamDesc,  0, 		%MaxIrq%
HKR, Ndi\Params\MaxInterrupt,   		Type,       0,      	"int"
HKR, Ndi\Params\MaxInterrupt,   		Base,       0,      	"10"
HKR, Ndi\Params\MaxInterrupt,   		Min,        0,       	"1000"
HKR, Ndi\Params\MaxInterrupt,   		Max,        0,       	"30000"
HKR, Ndi\Params\MaxInterrupt,   		Step,       0,      	"200"
HKR, Ndi\Params\MaxInterrupt,   		Default,    0,   	"5000"

HKR, Ndi\Params\MediaType,  			ParamDesc,  0,     	%MediaType%
HKR, Ndi\Params\MediaType,  			Type,       0,          "enum"
HKR, Ndi\Params\MediaType,  			Default,    0,       	"0"
HKR, Ndi\Params\MediaType\enum,     		"0",        0,   	%Auto%
HKR, Ndi\Params\MediaType\enum,     		"1",        0,   	%100MFD%
HKR, Ndi\Params\MediaType\enum,     		"2",        0,   	%100MHD%
HKR, Ndi\Params\MediaType\enum,     		"3",        0,   	%10MFD%
HKR, Ndi\Params\MediaType\enum,     		"4",        0,   	%10MHD%
HKR, Ndi\Params\MediaType\enum,     		"6",        0,   	%1GFD%

HKR, Ndi\Params\FlowControl,    		ParamDesc,  0,  	%FlowCtrl%
HKR, Ndi\Params\FlowControl,    		Type,       0,       	"enum"
HKR, Ndi\Params\FlowControl,    		Default,    0,    	"0"
HKR, Ndi\Params\FlowControl\enum, 		"1",        0,      	%On%
HKR, Ndi\Params\FlowControl\enum, 		"0",        0,      	%Off%

HKR, Ndi\Params\VLanID,				ParamDesc,  0,          %VLanID%
HKR, Ndi\Params\VLanID,   		        Base,       0,      	"10"
HKR, Ndi\Params\VLanID,				Type,	    0,          "long"
HKR, Ndi\Params\VLanID,				Min,        0,          "0"
HKR, Ndi\Params\VLanID,				Max,        0,          "4094"
HKR, Ndi\Params\VLanID,				Step,       0,          "1"
HKR, Ndi\Params\VLanID,				Default,    0,          "0"

[WOLDefault.params]
HKR, Ndi\Params\WakeUpCapability,   		ParamDesc,  0,     	%WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapability,   		Type,       0,          "enum"
HKR, Ndi\Params\WakeUpCapability,   		Default,    0,          "6"
HKR, Ndi\Params\WakeUpCapability\enum, 		"0",        0,          %None%
HKR, Ndi\Params\WakeUpCapability\enum, 		"1",        0,         	%LinkChange%
HKR, Ndi\Params\WakeUpCapability\enum, 		"2",        0,         	%MagicPacket%
HKR, Ndi\Params\WakeUpCapability\enum, 		"4",        0,         	%PatternMatch%
HKR, Ndi\Params\WakeUpCapability\enum, 		"3",        0,         	%Link_Magic%
HKR, Ndi\Params\WakeUpCapability\enum, 		"5",        0,         	%Link_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"6",        0,         	%Magic_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"7",        0,         	%All%

[WOLMagic.params]
HKR, Ndi\Params\WakeUpCapability,   		ParamDesc,  0,     	%WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapability,   		Type,       0,          "enum"
HKR, Ndi\Params\WakeUpCapability,   		Default,    0,          "2"
HKR, Ndi\Params\WakeUpCapability\enum, 		"0",        0,          %None%
HKR, Ndi\Params\WakeUpCapability\enum, 		"1",        0,         	%LinkChange%
HKR, Ndi\Params\WakeUpCapability\enum, 		"2",        0,         	%MagicPacket%
HKR, Ndi\Params\WakeUpCapability\enum, 		"4",        0,         	%PatternMatch%
HKR, Ndi\Params\WakeUpCapability\enum, 		"3",        0,         	%Link_Magic%
HKR, Ndi\Params\WakeUpCapability\enum, 		"5",        0,         	%Link_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"6",        0,         	%Magic_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"7",        0,         	%All%

[WOLNone.params]
HKR, Ndi\Params\WakeUpCapability,   		ParamDesc,  0,     	%WakeUpCapabilities%
HKR, Ndi\Params\WakeUpCapability,   		Type,       0,          "enum"
HKR, Ndi\Params\WakeUpCapability,   		Default,    0,          "0"
HKR, Ndi\Params\WakeUpCapability\enum, 		"0",        0,          %None%
HKR, Ndi\Params\WakeUpCapability\enum, 		"1",        0,         	%LinkChange%
HKR, Ndi\Params\WakeUpCapability\enum, 		"2",        0,         	%MagicPacket%
HKR, Ndi\Params\WakeUpCapability\enum, 		"4",        0,         	%PatternMatch%
HKR, Ndi\Params\WakeUpCapability\enum, 		"3",        0,         	%Link_Magic%
HKR, Ndi\Params\WakeUpCapability\enum, 		"5",        0,         	%Link_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"6",        0,         	%Magic_Pattern%
HKR, Ndi\Params\WakeUpCapability\enum, 		"7",        0,         	%All%

[Common.Params.WinNT]
HKR, Ndi\Params\LsoOffload,    			ParamDesc,  0, 		%LsoOff%
HKR, Ndi\Params\LsoOffload,    			Type,       0,      	"enum"
HKR, Ndi\Params\LsoOffload,    			Default,    0,   	"1"
HKR, Ndi\Params\LsoOffload\enum,		"1",        0,        	%On%
HKR, Ndi\Params\LsoOffload\enum,		"0",        0,        	%Off%

HKR, Ndi\Params\TCPChecksumOffloadIPv4,		ParamDesc,  0,  	%TCPChksumOffv4%
HKR, Ndi\Params\TCPChecksumOffloadIPv4,		Type,       0,       	"enum"
HKR, Ndi\Params\TCPChecksumOffloadIPv4,		Default,    0,     	"3"
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"3",        0,      	%TXRXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"2",        0,      	%RXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"1",        0,      	%TXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"0",        0,      	%Off%

HKR, Ndi\Params\IPChecksumOffloadIPv4,  	ParamDesc,  0,  	%IPChksumOffv4%
HKR, Ndi\Params\IPChecksumOffloadIPv4,  	Type,       0,       	"enum"
HKR, Ndi\Params\IPChecksumOffloadIPv4,          Default,    0,      	"3"
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"3",        0,       	%TXRXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"2",        0,       	%RXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"1",        0,       	%TXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"0",        0,       	%Off%

HKR, Ndi\Params\UDPChecksumOffloadIPv4,		ParamDesc,  0,  	%UDPChksumOffv4%
HKR, Ndi\Params\UDPChecksumOffloadIPv4,		Type,       0,       	"enum"
HKR, Ndi\Params\UDPChecksumOffloadIPv4,		Default,    0,     	"3"
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"3",        0,      	%TXRXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"2",        0,      	%RXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"1",        0,      	%TXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"0",        0,      	%Off%

HKR, Ndi\Params\MaxRxBuffer,    		ParamDesc,  0, 		%NumRx%
HKR, Ndi\Params\MaxRxBuffer,    		Type,       0,      	"int"
HKR, Ndi\Params\MaxRxBuffer,    		Base,       0,      	"10"
HKR, Ndi\Params\MaxRxBuffer,    		Min,        0,       	"16"
HKR, Ndi\Params\MaxRxBuffer,    		Max,        0,       	"2048"
HKR, Ndi\Params\MaxRxBuffer,    		Step,       0,      	"16"
HKR, Ndi\Params\MaxRxBuffer,    		Default,    0,   	"512"

HKR, Ndi\Params\MaxTxBuffer,    		ParamDesc,  0, 		%NumTx%
HKR, Ndi\Params\MaxTxBuffer,    		Type,       0,      	"int"
HKR, Ndi\Params\MaxTxBuffer,    		Base,       0,      	"10"
HKR, Ndi\Params\MaxTxBuffer,    		Min,        0,       	"16"
HKR, Ndi\Params\MaxTxBuffer,    		Max,        0,       	"1024"
HKR, Ndi\Params\MaxTxBuffer,    		Step,       0,      	"16"
HKR, Ndi\Params\MaxTxBuffer,    		Default,    0,   	"256"

[Pega.Params.WinNT]
HKR, Ndi\Params\LsoOffload,    			ParamDesc,  0, 		%LsoOff%
HKR, Ndi\Params\LsoOffload,    			Type,       0,      	"enum"
HKR, Ndi\Params\LsoOffload,    			Default,    0,   	"1"
HKR, Ndi\Params\LsoOffload\enum,		"1",        0,        	%On%
HKR, Ndi\Params\LsoOffload\enum,		"0",        0,        	%Off%

HKR, Ndi\Params\TCPChecksumOffloadIPv4,		ParamDesc,  0,  	%TCPChksumOffv4%
HKR, Ndi\Params\TCPChecksumOffloadIPv4,		Type,       0,       	"enum"
HKR, Ndi\Params\TCPChecksumOffloadIPv4,		Default,    0,     	"3"
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"3",        0,      	%TXRXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"2",        0,      	%RXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"1",        0,      	%TXEna%
HKR, Ndi\Params\TCPChecksumOffloadIPv4\enum,	"0",        0,      	%Off%

HKR, Ndi\Params\IPChecksumOffloadIPv4,  	ParamDesc,  0,  	%IPChksumOffv4%
HKR, Ndi\Params\IPChecksumOffloadIPv4,  	Type,       0,       	"enum"
HKR, Ndi\Params\IPChecksumOffloadIPv4,          Default,    0,      	"3"
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"3",        0,       	%TXRXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"2",        0,       	%RXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"1",        0,       	%TXEna%
HKR, Ndi\Params\IPChecksumOffloadIPv4\enum,	"0",        0,       	%Off%

HKR, Ndi\Params\UDPChecksumOffloadIPv4,		ParamDesc,  0,  	%UDPChksumOffv4%
HKR, Ndi\Params\UDPChecksumOffloadIPv4,		Type,       0,       	"enum"
HKR, Ndi\Params\UDPChecksumOffloadIPv4,		Default,    0,     	"3"
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"3",        0,      	%TXRXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"2",        0,      	%RXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"1",        0,      	%TXEna%
HKR, Ndi\Params\UDPChecksumOffloadIPv4\enum,	"0",        0,      	%Off%

HKR, Ndi\Params\MaxRxBuffer,    		ParamDesc,  0, 		%NumRx%
HKR, Ndi\Params\MaxRxBuffer,    		Type,       0,      	"int"
HKR, Ndi\Params\MaxRxBuffer,    		Base,       0,      	"10"
HKR, Ndi\Params\MaxRxBuffer,    		Min,        0,       	"16"
HKR, Ndi\Params\MaxRxBuffer,    		Max,        0,       	"2048"
HKR, Ndi\Params\MaxRxBuffer,    		Step,       0,      	"16"
HKR, Ndi\Params\MaxRxBuffer,    		Default,    0,   	"1024"

HKR, Ndi\Params\MaxTxBuffer,    		ParamDesc,  0, 		%NumTx%
HKR, Ndi\Params\MaxTxBuffer,    		Type,       0,      	"int"
HKR, Ndi\Params\MaxTxBuffer,    		Base,       0,      	"10"
HKR, Ndi\Params\MaxTxBuffer,    		Min,        0,       	"16"
HKR, Ndi\Params\MaxTxBuffer,    		Max,        0,       	"1024"
HKR, Ndi\Params\MaxTxBuffer,    		Step,       0,      	"16"
HKR, Ndi\Params\MaxTxBuffer,    		Default,    0,   	"256"

[ShutOn.params]
HKR, Ndi\Params\ShutdownWake,   		ParamDesc,  0, 		%ShutDW%
HKR, Ndi\Params\ShutdownWake,   		Type,       0,      	"enum"
HKR, Ndi\Params\ShutdownWake,   		Default,    0,   	"1"
HKR, Ndi\Params\ShutdownWake\enum,		"1",        0,       	%On%
HKR, Ndi\Params\ShutdownWake\enum,		"0",        0,       	%Off%

[ShutOff.params]
HKR, Ndi\Params\ShutdownWake,   		ParamDesc,  0, 		%ShutDW%
HKR, Ndi\Params\ShutdownWake,   		Type,       0,      	"enum"
HKR, Ndi\Params\ShutdownWake,   		Default,    0,   	"0"
HKR, Ndi\Params\ShutdownWake\enum,		"1",        0,       	%On%
HKR, Ndi\Params\ShutdownWake\enum,		"0",        0,       	%Off%

[EEELPI.params]
HKR, Ndi\Params\EEESupported,                   ParamDesc,  0,          "AZPower"
HKR, Ndi\Params\EEESupported,                   Type,       0,          "enum"
HKR, Ndi\Params\EEESupported,                   Default,    0,          "0"
HKR, Ndi\Params\EEESupported\enum,              "1",        0,          %On%
HKR, Ndi\Params\EEESupported\enum,              "0",        0,          %Off%

[EEELPIEn.params]
HKR, Ndi\Params\EEESupported,                   ParamDesc,  0,          "AZPower"
HKR, Ndi\Params\EEESupported,                   Type,       0,          "enum"
HKR, Ndi\Params\EEESupported,                   Default,    0,          "1"
HKR, Ndi\Params\EEESupported\enum,              "1",        0,          %On%
HKR, Ndi\Params\EEESupported\enum,              "0",        0,          %Off%
;-----------------------------------------------------------------------------
; DestinationDirs
;
[L1c.CopyFiles]
l1c51x86.sys,,,2

[SourceDisksNames]
;
; diskid = description[, [tagfile] [, <unused>, subdir]]
;
1 = %DriverDisk%,,,

[SourceDisksFiles]
;
; filename_on_source = diskID[, [subdir][, size]]
;
l1c51x86.sys = 1

[DestinationDirs]
L1c.CopyFiles   = 12
DefaultDestDir  = 11

[Strings]
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo Frame"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS mode"
AZPower                 = "802.3az"
NetAddr         	= "Network Address"
MTU             	= "Maximum Frame Size"
TOff            	= "Task Offload"
MaxIrq          	= "Max IRQ per Second"
NumRx           	= "Number of Rx Buffers"
NumTx           	= "Number of Tx Buffers"
FlowCtrl        	= "Flow Control"
ShutDW          	= "Shutdown Wakeup"
MediaType       	= "MediaType"
Auto            	= "Auto"
1GFD                    = "1.0 Gbps Full Duplex"
10MHD           	= "10Mbps Half Duplex"
10MFD           	= "10Mbps Full Duplex"
100MHD          	= "100Mbps Half Duplex"
100MFD          	= "100Mbps Full Duplex"
WakeUpCapabilities      = "WakeUp Capabilities"
None            	= "None"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "All"
On              	= "On"
Off             	= "Off"
TXEna 			= "Tx Enabled"
RXEna 			= "Rx Enabled"
TXRXEna 		= "Tx & Rx Enabled"
IPChksumOffv4 		= "IPv4 Checksum Offload"
TCPChksumOffv4 		= "TCP Checksum Offload (IPv4)"
UDPChksumOffv4 		= "UDP Checksum Offload (IPv4)"
LsoOff                  = "Large Send Offload"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Chinese (Taiwan)
[Strings.0404]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "大型框架"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS 模式"
AZPower                 = "802.3az"
NetAddr         	= "網路位址"
MTU             	= "框架大小上限"
TOff            	= "作業卸載"
MaxIrq          	= "每秒 IRQ 上限"
NumRx           	= "接收緩衝數量"
NumTx           	= "傳輸緩衝數量"
FlowCtrl        	= "流量控制"
ShutDW          	= "關閉狀態喚醒"
MediaType       	= "MediaType"
Auto            	= "自動"
1GFD                    = "1.0 Gbps 全雙工"
10MHD           	= "10Mbps 半雙工"
10MFD           	= "10Mbps 全雙工"
100MHD          	= "100Mbps 半雙工"
100MFD          	= "100Mbps 全雙工"
WakeUpCapabilities      = "喚醒功能"
None            	= "無"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "全部"
On              	= "開啟"
Off             	= "關閉"
TXEna 			= "傳輸已啟用"
RXEna 			= "接收已啟用"
TXRXEna 		= "傳輸和接收已啟用"
IPChksumOffv4 		= "IPv4 檢查總和卸載"
TCPChksumOffv4 		= "TCP 檢查總和卸載 (IPv4)"
UDPChksumOffv4 		= "UDP 檢查總和卸載 (IPv4)"
LsoOff                  = "大型傳送卸載"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; German (Standard)
[Strings.0407]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo-Frame"
2KBMTU      		= "2 KB MTU"
3KBMTU      		= "3 KB MTU"
4KBMTU      		= "4 KB MTU"
5KBMTU      		= "5 KB MTU"
6KBMTU      		= "6 KB MTU"
7KBMTU      		= "7 KB MTU"
8KBMTU      		= "8 KB MTU"
9KBMTU      		= "9 KB MTU"
APSmode			= "APS-Modus"
AZPower                 = "802.3az"
NetAddr         	= "Netzwerkadresse"
MTU             	= "Maximale Framegröße"
TOff            	= "Task-Offload"
MaxIrq          	= "Max. IRQ pro Sekunde"
NumRx           	= "Anzahl Rx-Puffer"
NumTx           	= "Anzahl Tx-Puffer"
FlowCtrl        	= "Flusssteuerung"
ShutDW          	= "Shutdown/Wakeup"
MediaType       	= "MediaType"
Auto            	= "Automatisch"
1GFD                     = "1.0 Gbit/s Vollduplex"
10MHD           	= "10 Mbit/s Halbduplex"
10MFD           	= "10 Mbit/s Vollduplex"
100MHD          	= "100 Mbit/s Halbduplex"
100MFD          	= "100 Mbit/s Vollduplex"
WakeUpCapabilities      = "WakeUp-Eigenschaften"
None            	= "Keine"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "Alle"
On              	= "An"
Off             	= "Aus"
TXEna 			= "Tx aktiviert"
RXEna 			= "Rx aktiviert"
TXRXEna 		= "Tx & Rx aktiviert"
IPChksumOffv4 		= "IPv4 Checksum Offload"
TCPChksumOffv4 		= "TCP Checksum Offload (IPv4)"
UDPChksumOffv4 		= "UDP Checksum Offload (IPv4)"
LsoOff                  = "Large Send Offload"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Spanish (Spain, Traditional Sort)
[Strings.040A]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Trama gigante"
2KBMTU      		= "MTU de 2KB"
3KBMTU      		= "MTU de 3KB"
4KBMTU      		= "MTU de 4KB"
5KBMTU      		= "MTU de 5KB"
6KBMTU      		= "MTU de 6KB"
7KBMTU      		= "MTU de 7KB"
8KBMTU      		= "MTU de 8KB"
9KBMTU      		= "MTU de 9KB"
APSmode			= "Modo APS"
AZPower                 = "802.3az"
NetAddr         	= "Dirección de red"
MTU             	= "Tamaño máximo de trama"
TOff            	= "Descarga de tarea"
MaxIrq          	= "IRQ máx por segundo"
NumRx           	= "Número de búfers de recepción"
NumTx           	= "Número de búfers de transmisión"
FlowCtrl        	= "Control de flujo"
ShutDW          	= "Reactivar cierre"
MediaType       	= "MediaType"
Auto            	= "Automático"
1GFD                    = "Dúplex completo 1.0Gbps"
10MHD           	= "Dúplex medio 10Mbps"
10MFD           	= "Dúplex completo 10Mbps"
100MHD          	= "Dúplex medio 100Mbps"
100MFD          	= "Dúplex completo 100Mbps"
WakeUpCapabilities      = "Capacidades de reactivación"
None            	= "Ninguno"
LinkChange      	= "Link Change"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Pattern Match"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "Todo"
On              	= "Activado"
Off             	= "Desactivado"
TXEna 			= "Transmisión habilitada"
RXEna 			= "Recepción habilitada"
TXRXEna 		= "Transmisión y recepción habilitadas"
IPChksumOffv4 		= "Carga de suma de comprobación IPv4"
TCPChksumOffv4 		= "Carga de suma de comprobación TCP (IPv4)"
UDPChksumOffv4 		= "Carga de suma de comprobación UDP (IPv4)"
LsoOff                  = "Gran carga de envío"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; French (Standard)
[Strings.040C]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Trame Jumbo"
2KBMTU      		= "MTU de 2 Ko"
3KBMTU      		= "MTU de 3 Ko"
4KBMTU      		= "MTU de 4 Ko"
5KBMTU      		= "MTU de 5 Ko"
6KBMTU      		= "MTU de 6 Ko"
7KBMTU      		= "MTU de 7 Ko"
8KBMTU      		= "MTU de 8 Ko"
9KBMTU      		= "MTU de 9 Ko"
APSmode			= "Mode APS"
AZPower                 = "802.3az"
NetAddr         	= "Adresse réseau"
MTU             	= "Taille maximale de la trame "
TOff            	= "Déchargement de tâche"
MaxIrq          	= "IRQ maxi. par seconde"
NumRx           	= "Nombre de tampons rx"
NumTx           	= "Nombre de tampons Tx"
FlowCtrl        	= "Contrôle de flux"
ShutDW          	= "Sortie de veille à l'arrêt"
MediaType       	= "MediaType"
Auto            	= "Automatique"
1GFD                    = "1.0 Gbits/s Duplex intégral"
10MHD           	= "10 Mbits/s Semi-duplex"
10MFD           	= "10 Mbits/s Duplex intégral"
100MHD          	= "100 Mbits/s Semi-duplex"
100MFD          	= "100 Mbits/s Duplex intégral"
WakeUpCapabilities      = "Capacités de mise en éveil"
None            	= "Aucune"
LinkChange      	= "Changement de liaison"
MagicPacket     	= "Paquet magique"
PatternMatch    	= "Correspondance au modèle"
Link_Magic      	= "LinkChange et MagicPacket"
Link_Pattern    	= "LinkChange et PatternMatch"
Magic_Pattern   	= "MagicPack et PatternMatch"
All             	= "Tous"
On              	= "Activé"
Off             	= "Désactivé"
TXEna 			= "Tx activé"
RXEna 			= "Rx activé"
TXRXEna 		= "Tx et rx activés"
IPChksumOffv4 		= "Déchargement de somme de contrôle IPv4"
TCPChksumOffv4 		= "Déchargement de somme de contrôle TCP (IPv4)"
UDPChksumOffv4 		= "Déchargement de somme de contrôle UDP (IPv4)"
LsoOff                  = "Déchargement d'envoi important"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Italian (Standard)
[Strings.0410]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Frame jumbo"
2KBMTU      		= "MTU 2 KB"
3KBMTU      		= "MTU 3 KB"
4KBMTU      		= "MTU 4 KB"
5KBMTU      		= "MTU 5 KB"
6KBMTU      		= "MTU 6 KB"
7KBMTU      		= "MTU 7 KB"
8KBMTU      		= "MTU 8 KB"
9KBMTU      		= "MTU 9 KB"
APSmode			= "Modalità APS"
AZPower                 = "802.3az"
NetAddr         	= "Indirizzo di rete"
MTU             	= "Dimensioni massime frame"
TOff            	= "Offload attività"
MaxIrq          	= "Numero massimo di IRQ per secondo"
NumRx           	= "Numero di buffer Rx"
NumTx           	= "Numero di buffer Tx"
FlowCtrl        	= "Controllo di flusso"
ShutDW          	= "Attivazione arresto"
MediaType       	= "MediaType"
Auto            	= "Automatica"
1GFD                    = "Full Duplex 1.0 Gbps"
10MHD           	= "Half Duplex 10 Mbps"
10MFD           	= "Full Duplex 10 Mbps"
100MHD          	= "Half Duplex 100 Mbps"
100MFD          	= "Full Duplex 100 Mbps"
WakeUpCapabilities      = "Capacità di attivazione"
None            	= "Nessuno"
LinkChange      	= "Modifica collegamento"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Corrispondenza motivo"
Link_Magic      	= "LinkChange e MagicPacket"
Link_Pattern    	= "LinkChange e PatternMatch"
Magic_Pattern   	= "MagicPacket e PatternMatch"
All             	= "Tutti"
On              	= "On"
Off             	= "Off"
TXEna 			= "Tx attivato"
RXEna 			= "Rx attivato"
TXRXEna 		= "Abilitato Tx e Rx"
IPChksumOffv4 		= "Offload checksum IPv4"
TCPChksumOffv4 		= "Offload di checksum TCP (IPv4)"
UDPChksumOffv4 		= "Offload di checksum UDP (IPv4)"
LsoOff                  = "Offload invio di grandi dimensioni"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Japanese
[Strings.0411]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "ジャンボ フレーム"
2KBMTU      		= "2 KB MTU"
3KBMTU      		= "3 KB MTU"
4KBMTU      		= "4 KB MTU"
5KBMTU      		= "5 KB MTU"
6KBMTU      		= "6 KB MTU"
7KBMTU      		= "7 KB MTU"
8KBMTU      		= "8 KB MTU"
9KBMTU      		= "9 KB MTU"
APSmode			= "APS モード"
AZPower                 = "802.3az"
NetAddr         	= "ネットワーク アドレス"
MTU             	= "最大フレーム サイズ"
TOff            	= "タスク オフロード"
MaxIrq          	= "最大 IRQ/秒"
NumRx           	= "Rx バッファ数"
NumTx           	= "Tx バッファ数"
FlowCtrl        	= "フロー制御"
ShutDW          	= "シャットダウン ウェークアップ"
MediaType       	= "MediaType"
Auto            	= "自動"
1GFD                    = "1.0 Gbps 全二重"
10MHD           	= "10 Mbps 半二重"
10MFD           	= "10 Mbps 全二重"
100MHD          	= "100 Mbps 半二重"
100MFD          	= "100 Mbps 全二重"
WakeUpCapabilities      = "ウェークアップ機能"
None            	= "なし"
LinkChange      	= "リンク変更"
MagicPacket     	= "マジック パケット"
PatternMatch    	= "パターン マッチ"
Link_Magic      	= "LinkChange と MagicPacket"
Link_Pattern    	= "LinkChange と PatternMatch"
Magic_Pattern   	= "MagicPacket と PatternMatch"
All             	= "すべて"
On              	= "オン"
Off             	= "オフ"
TXEna 			= "Tx 有効化"
RXEna 			= "Rx 有効化"
TXRXEna 		= "Tx と Rx の有効化"
IPChksumOffv4 		= "IPv4 チェックサム オフロード"
TCPChksumOffv4 		= "TCP チェックサム オフロード (IPv4)"
UDPChksumOffv4 		= "UDP チェックサム オフロード (IPv4)"
LsoOff                  = "大量送信オフロード"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Dutch (Netherlands)
[Strings.0413]
;; Do NOT translate
;---------------------------------------------------------------------------------------------------
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumboframe"
2KBMTU      		= "2 KB MTU"
3KBMTU      		= "3 KB MTU"
4KBMTU      		= "4 KB MTU"
5KBMTU      		= "5 KB MTU"
6KBMTU      		= "6 KB MTU"
7KBMTU      		= "7 KB MTU"
8KBMTU      		= "8 KB MTU"
9KBMTU      		= "9 KB MTU"
APSmode			= "APS-modus"
AZPower                 = "802.3az"
NetAddr         	= "Netwerkadres"
MTU             	= "Maximale framegrootte"
TOff            	= "Offload van taken"
MaxIrq          	= "Max. IRQ per seconde"
NumRx           	= "Aantal Rx-buffers"
NumTx           	= "Aantal Tx-buffers"
FlowCtrl        	= "Datatransportbesturing"
ShutDW          	= "Afsluiten Ontwaken"
MediaType       	= "MediaType"
Auto            	= "Automatisch"
1GFD                    = "1.0 Gbps volledige duplex"
10MHD           	= "10 Mbps half-duplex"
10MFD           	= "10 Mbps volledige duplex"
100MHD          	= "100 Mbps half-duplex"
100MFD          	= "100 Mbps volledige duplex"
WakeUpCapabilities      = "Mogelijkheden voor ontwaken"
None            	= "Geen"
LinkChange      	= "Wijziging koppeling"
MagicPacket     	= "Magic-pakket"
PatternMatch    	= "Patroonovereenkomst"
Link_Magic      	= "Wijziging koppeling en Magic-pakket"
Link_Pattern    	= "Wijziging koppeling en Patroonovereenkomst"
Magic_Pattern   	= "Magic-pakket en Patroonovereenkomst"
All             	= "Alles"
On              	= "Aan"
Off             	= "Uit"
TXEna 			= "Tx ingeschakeld"
RXEna 			= "Rx ingeschakeld"
TXRXEna 		= "Tx en Rx ingeschakeld"
IPChksumOffv4 		= "Offload van IPv4-controlesom"
TCPChksumOffv4 		= "Offload van TCP-controlesom (IPv4)"
UDPChksumOffv4 		= "Offload van UDP-controlesom (IPv4)"
LsoOff                  = "Grote verzendings-offload"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

;; Do NOT translate
;---------------------------------------------------------------------------------------------------
; Portuguese (Brazil)
[Strings.0416]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo Frame"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "Modo APS"
AZPower                 = "802.3az"
NetAddr         	= "Endereço de Rede"
MTU             	= "Tamanho Máximo do Pacote"
TOff            	= "Descarga de Tarefas"
MaxIrq          	= "Max IRQ por Segundo"
NumRx           	= "Número de Rx Buffers"
NumTx           	= "Número de Tx Buffers"
FlowCtrl        	= "Controlo d Fluxo"
ShutDW          	= "Encerramento Reactivação"
MediaType       	= "MediaType"
Auto            	= "Automático"
1GFD                    = "1.0 Gbps Full Duplex"
10MHD           	= "10Mbps Half Duplex"
10MFD           	= "10Mbps Full Duplex"
100MHD          	= "100Mbps Half Duplex"
100MFD          	= "100Mbps Full Duplex"
WakeUpCapabilities      = "Capacidades de Reactivação"
None            	= "Nenhum"
LinkChange      	= "Alteração de Ligação"
MagicPacket     	= "Magic Packet"
PatternMatch    	= "Correspondência por Padrão"
Link_Magic      	= "Alteração de Ligação e MagicPacket"
Link_Pattern    	= "Alteração de Ligação e Correspondência por Padrão"
Magic_Pattern   	= "MagicPacket e Correspondência por Padrão"
All             	= "Todos"
On              	= "Ligado"
Off             	= "Desligado"
TXEna 			= "Tx Activada"
RXEna 			= "Rx Activada"
TXRXEna 		= "Tx e Rx Activadas"
IPChksumOffv4 		= "IPv4 Checksum Offload"
TCPChksumOffv4 		= "TCP Checksum Offload (IPv4)"
UDPChksumOffv4 		= "UDP Checksum Offload (IPv4)"
LsoOff                  = "Large Send Offload"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Chinese (PRC)
[Strings.0804]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo 帧"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS 模式"
AZPower                 = "802.3az"
NetAddr         	= "网络地址"
MTU             	= "最大帧大小"
TOff            	= "任务卸载"
MaxIrq          	= "每秒最大 IRQ"
NumRx           	= "Rx 缓冲区数"
NumTx           	= "Tx 缓冲区数"
FlowCtrl        	= "流控制"
ShutDW          	= "关闭状态唤醒"
MediaType       	= "MediaType"
Auto            	= "自动"
1GFD                    = "1.0 Gbps 全双工"
10MHD           	= "10Mbps 半双工"
10MFD           	= "10Mbps 全双工"
100MHD          	= "100Mbps 半双工"
100MFD          	= "100Mbps 全双工"
WakeUpCapabilities      = "唤醒功能"
None            	= "无"
LinkChange      	= "链接更改"
MagicPacket     	= "幻数据包"
PatternMatch    	= "模式匹配"
Link_Magic      	= "LinkChange & MagicPacket"
Link_Pattern    	= "LinkChange & PatternMatch"
Magic_Pattern   	= "MagicPacket & PatternMatch"
All             	= "全部"
On              	= "开"
Off             	= "关"
TXEna 			= "Tx 已启用"
RXEna 			= "Rx 已启用"
TXRXEna 		= "Tx 和 Rx 已启用"
IPChksumOffv4 		= "IPv4 校验和卸载"
TCPChksumOffv4 		= "TCP 校验和卸载 (IPv4)"
UDPChksumOffv4 		= "UDP 校验和卸载 (IPv4)"
LsoOff                  = "大量发送卸载"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Czech
[Strings.0405]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo Frame"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "Režim APS"
AZPower                 = "802.3az"
NetAddr         	= "Adresa sítě"
MTU             	= "Maximální velikost rámce"
TOff            	= "Snížení pracovní zátěže"
MaxIrq          	= "Maximální počet IRQ za vteřinu"
NumRx           	= "Množství vyrovnávací paměti Rx"
NumTx           	= "Množství vyrovnávací paměti Tx"
FlowCtrl        	= "Řízení toku"
ShutDW          	= "Probuzení vypnutého počítače"
MediaType       	= "Druh média"
Auto		  	= "Automatické vyjednávání"
1GFD                    = "Plný duplex 1.0 Gb/s"
10MHD		  	= "Poloviční duplex 10 Mb/s"
10MFD		  	= "Plný duplex 10 Mb/s"
100MHD			= "Poloviční duplex 100 Mb/s"
100MFD			= "Plný duplex 100 Mb/s"
WakeUpCapabilities      = "Schopnosti probuzení počítače"
None            	= "Žádný"
LinkChange      	= "Změna linky"
MagicPacket     	= "Magický paket"
PatternMatch    	= "Porovnávací vzorek"
Link_Magic      	= "Změna linky a magický paket"
Link_Pattern    	= "Změna linky a porovnávací vzorek"
Magic_Pattern   	= "Magický paket a porovnávací vzorek"
All             	= "Vše"
On              	= "Zapnuto"
Off             	= "Vypnuto"
TXEna 			= "Tx zapnuto"
RXEna 			= "Rx zapnuto"
TXRXEna 		= "Tx a Rx zapnuto"
IPChksumOffv4 		= "Odstranění kontrolního součtu u protokolu IPv4"
TCPChksumOffv4 		= "Odstranění kontrolního součtu u protokolu TCP (IPv4)"
UDPChksumOffv4 		= "Odstranění kontrolního součtu u protokolu UDP (IPv4)"
LsoOff                  = "Snižování zátěže u rozsáhlého odesílání"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Danish
[Strings.0406]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumboramme"
2KBMTU      		= "2 KB MTU"
3KBMTU      		= "3 KB MTU"
4KBMTU      		= "4 KB MTU"
5KBMTU      		= "5 KB MTU"
6KBMTU      		= "6 KB MTU"
7KBMTU      		= "7 KB MTU"
8KBMTU      		= "8 KB MTU"
9KBMTU      		= "9 KB MTU"
APSmode			= "APS-tilstand"
AZPower                 = "802.3az"
NetAddr         	= "Netværksadresse"
MTU             	= "Maksimal rammestørrelse"
TOff            	= "Aflastning af opgave"
MaxIrq          	= "Maks. IRQ pr. sekund"
NumRx           	= "Antal Rx-buffere"
NumTx           	= "Antal Tx-buffere"
FlowCtrl        	= "FlowControl"
ShutDW          	= "Lukning/aktivering"
MediaType       	= "Medietype"
Auto		  	= "Automatisk forhandling"
1GFD                    = "1.0 Gbps fuld duplex"
10MHD		  	= "10 Mbps halv duplex"
10MFD		  	= "10 Mbps fuld duplex"
100MHD			= "100 Mbps halv duplex"
100MFD			= "100 Mbps fuld duplex"
WakeUpCapabilities      = "Aktiveringsfunktioner"
None            	= "Ingen"
LinkChange      	= "Forbindelsesændring"
MagicPacket     	= "Magisk pakke"
PatternMatch    	= "Mønstermatch"
Link_Magic      	= "Forbindelsesændring og magisk pakke"
Link_Pattern    	= "Forbindelsesændring og mønstermatch"
Magic_Pattern   	= "Magisk pakke og mønstermatch"
All             	= "Alt"
On              	= "Til"
Off             	= "Fra"
TXEna 			= "Tx-aktiveret"
RXEna 			= "Rx-aktiveret"
TXRXEna 		= "Tx- og Rx-aktiveret"
IPChksumOffv4 		= "Aflastning af IPv4-kontrolsum"
TCPChksumOffv4 		= "Aflastning af TCP-kontrolsum (IPv4)"
UDPChksumOffv4 		= "Aflastning af UDP-kontrolsum (IPv4)"
LsoOff                  = "Aflastning af for stor forsendelse"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Finnish
[Strings.040b]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo-kehys"
2KBMTU      		= "2 kt MTU"
3KBMTU      		= "3 kt MTU"
4KBMTU      		= "4 kt MTU"
5KBMTU      		= "5 kt MTU"
6KBMTU      		= "6 kt MTU"
7KBMTU      		= "7 kt MTU"
8KBMTU      		= "8 kt MTU"
9KBMTU      		= "9 kt MTU"
APSmode			= "Yhteyspistepalvelutila"
AZPower                 = "802.3az"
NetAddr         	= "Verkko-osoite"
MTU             	= "Kehyksen maksimikoko"
TOff            	= "Tehtävän purku"
MaxIrq          	= "Enintään IRQ/s"
NumRx           	= "Rx-puskureiden lukumäärä"
NumTx           	= "Tx-puskureiden lukumäärä"
FlowCtrl        	= "Vuonohjaus"
ShutDW          	= "Herätys sammutuksesta"
MediaType       	= "Tietovälinelaji"
Auto		  	= "Automaattinen neuvottelu"
1GFD                    = "1.0 Gbps kaksisuuntaisuus"
10MHD		  	= "10 Mbps vuorosuuntaisuus"
10MFD		  	= "10 Mbps kaksisuuntaisuus"
100MHD			= "100 Mbps vuorosuuntaisuus"
100MFD			= "100 Mbps kaksisuuntaisuus"
WakeUpCapabilities      = "Heräämisominaisuudet"
None            	= "Ei mitään"
LinkChange      	= "Linkin vaihto"
MagicPacket     	= "Magic-paketti"
PatternMatch    	= "Mallivastaavuus"
Link_Magic      	= "Linkin vaihto & magic-paketti"
Link_Pattern    	= "Linkin vaihto & mallivastaavuus"
Magic_Pattern   	= "Magic-paketti & mallivastaavuus"
All             	= "Kaikki"
On              	= "Käytössä"
Off             	= "Pois käytöstä"
TXEna 			= "Tx käytössä"
RXEna 			= "Rx käytössä"
TXRXEna 		= "Tx & Rx käytössä"
IPChksumOffv4 		= "IPv4-tarkistussumman purku"
TCPChksumOffv4 		= "TCP-tarkistussumman purku (IPv4)"
UDPChksumOffv4 		= "UDP-tarkistussumman purku (IPv4)"
LsoOff                  = "Suuren lähetyksen purku"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Greek
[Strings.0408]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Πλαίσιο Jumbo"
2KBMTU      		= "2 KB MTU"
3KBMTU      		= "3 KB MTU"
4KBMTU      		= "4 KB MTU"
5KBMTU      		= "5 KB MTU"
6KBMTU      		= "6 KB MTU"
7KBMTU      		= "7 KB MTU"
8KBMTU      		= "8 KB MTU"
9KBMTU      		= "9 KB MTU"
APSmode			= "Λειτουργία APS"
AZPower                 = "802.3az"
NetAddr         	= "Διεύθυνση δικτύου"
MTU             	= "Μέγιστο μέγεθος πλαισίου"
TOff            	= "Μείωση φόρτου εργασίας"
MaxIrq          	= "Μέγιστος αριθμός IRQ ανά δευτερόλεπτο"
NumRx           	= "Αριθμός καταχωρητών Rx"
NumTx           	= "Αριθμός καταχωρητών Tx"
FlowCtrl        	= "Έλεγχος ροής"
ShutDW          	= "Ενεργοποίηση τερματισμού"
MediaType       	= "Τύπος μέσου"
Auto		  	= "Αυτόματη διαπραγμάτευση"
1GFD                    = "Πλήρως αμφίδρομο 1.0 Gbps"
10MHD		  	= "Ημι-αμφίδρομο 10 Mbps"
10MFD		  	= "Πλήρως αμφίδρομο 10 Mbps"
100MHD			= "Ημι-αμφίδρομο 100 Mbps"
100MFD			= "Πλήρως αμφίδρομο 100 Mbps"
WakeUpCapabilities      = "Δυνατότητες ενεργοποίησης"
None            	= "Χωρίς"
LinkChange	        = "Αλλαγή σύνδεσης"
MagicPacket	        = "Μαγικό πακέτο"
PatternMatch	        = "Ταίριασμα μοτίβου"
Link_Magic      	= "Αλλαγή σύνδεσης & Μαγικό πακέτο"
Link_Pattern    	= "Αλλαγή σύνδεσης & ταίριασμα μοτίβου"
Magic_Pattern   	= "Μαγικό πακέτο & ταίριασμα μοτίβου"
All             	= "Όλα"
On              	= "Ενεργοποίηση"
Off             	= "Απενεργοποίηση"
TXEna 			= "Ενεργοποιημένο Tx"
RXEna 			= "Ενεργοποιημένο Rx"
TXRXEna 		= "Ενεργοποιημένο Tx & Rx"
IPChksumOffv4 		= "Μείωση φόρτου αθροίσματος ελέγχου IPv4"
TCPChksumOffv4 		= "Μείωση φόρτου αθροίσματος ελέγχου TCP (IPv4)"
UDPChksumOffv4 		= "Μείωση φόρτου αθροίσματος ελέγχου UDP (IPv4)"
LsoOff                  = "Μείωση φόρτου μεγάλης αποστολής"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Hungarian
[Strings.040e]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Óriáskeret"
2KBMTU      		= "2 kB MTU"
3KBMTU      		= "3 kB MTU"
4KBMTU      		= "4 kB MTU"
5KBMTU      		= "5 kB MTU"
6KBMTU      		= "6 kB MTU"
7KBMTU      		= "7 kB MTU"
8KBMTU      		= "8 kB MTU"
9KBMTU      		= "9 kB MTU"
APSmode			= "APS mód"
AZPower                 = "802.3az"
NetAddr         	= "Hálózati cím"
MTU             	= "Maximális keretméret"
TOff            	= "Feladat kihelyezése"
MaxIrq          	= "Másodpercenkénti maximális IRQ"
NumRx           	= "Fogadási pufferek száma"
NumTx           	= "Átviteli pufferek száma"
FlowCtrl        	= "Forgalomszabályozás"
ShutDW          	= "Felébresztés"
MediaType       	= "Hordozótípus"
Auto		  	= "Automatikus egyeztetés"
1GFD                    = "1.0 Gbps-os teljes duplex"
10MHD		  	= "10 Mbps-os fél duplex"
10MFD		  	= "10 Mbps-os teljes duplex"
100MHD			= "100 Mbps-os fél duplex"
100MFD			= "100 Mbps-os teljes duplex"
WakeUpCapabilities      = "Ébresztési szolgáltatások"
None            	= "Nincs"
LinkChange	        = "Csatolásállapot-változás"
MagicPacket	        = "Bűvös csomag"
PatternMatch	        = "Mintaegyezés"
Link_Magic      	= "Csatolásállapot-változás és Bűvös csomag"
Link_Pattern    	= "Csatolásállapot-változás és mintaegyezés"
Magic_Pattern   	= "Bűvös csomag és mintaegyezés"
All             	= "Összes"
On              	= "Be"
Off             	= "Ki"
TXEna 			= "Tx engedélyezve"
RXEna 			= "Rx engedélyezve"
TXRXEna 		= "Tx és Rx engedélyezve"
IPChksumOffv4 		= "IPv4 ellenőrző összeg számításának kihelyezése"
TCPChksumOffv4 		= "TCP ellenőrző összeg számításának kihelyezése (IPv4)"
UDPChksumOffv4 		= "UDP ellenőrző összeg számításának kihelyezése (IPv4)"
LsoOff                  = "Tehermentesítés nagy méretű küldés esetén"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Korean
[Strings.0412]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo 프레임"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS 모드"
AZPower                 = "802.3az"
NetAddr         	= "네트워크 주소"
MTU             	= "최대 프레임 크기"
TOff            	= "작업 오프로드"
MaxIrq          	= "초당 최대 IRQ"
NumRx           	= "수신 버퍼 수"
NumTx           	= "전송 버퍼 수"
FlowCtrl        	= "흐름 제어(FlowControl)"
ShutDW          	= "중지 모드 해제(Shutdown Wake Up)"
MediaType       	= "미디어 유형(MediaType)"
Auto		  	= "자동 협상"
1GFD                    = "1.0 Gbps 전이중"
10MHD		  	= "10Mbps 반이중"
10MFD		  	= "10Mbps 전이중"
100MHD			= "100Mbps 반이중"
100MFD			= "100Mbps 전이중"
WakeUpCapabilities      = "절전 모드 해제 기능"
None            	= "없음"
LinkChange	        = "연결 변경"
MagicPacket	        = "매직 패킷"
PatternMatch	        = "패턴 일치"
Link_Magic      	= "연결 변경 및 매직 패킷"
Link_Pattern    	= "연결 변경 및 패턴 일치"
Magic_Pattern   	= "매직 패킷 및 패턴 일치"
All             	= "전체"
On              	= "켜짐"
Off             	= "꺼짐"
TXEna 			= "Tx 사용"
RXEna 			= "Rx 사용"
TXRXEna 		= "Tx 및 Rx 사용"
IPChksumOffv4 		= "IPv4 체크섬 오프로드"
TCPChksumOffv4 		= "TCP 체크섬 오프로드(IPv4)"
UDPChksumOffv4 		= "UDP 체크섬 오프로드(IPv4)"
LsoOff                  = "Large Send Offload"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Norwegian
[Strings.0414]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo Frame"
2KBMTU      		= "2 kB MTU"
3KBMTU      		= "3 kB MTU"
4KBMTU      		= "4 kB MTU"
5KBMTU      		= "5 kB MTU"
6KBMTU      		= "6 kB MTU"
7KBMTU      		= "7 kB MTU"
8KBMTU      		= "8 kB MTU"
9KBMTU      		= "9 kB MTU"
APSmode			= "APS-modus"
AZPower                 = "802.3az"
NetAddr         	= "Nettverksadresse"
MTU             	= "Maksimal rammestørrelse"
TOff            	= "Oppgaveavlasting"
MaxIrq          	= "Maks. IRQ per sekund"
NumRx           	= "Antall Rx-buffere"
NumTx           	= "Antall Tx-buffere"
FlowCtrl        	= "Flytkontroll"
ShutDW          	= "Deaktiver oppvåkning"
MediaType       	= "Medietype"
Auto		  	= "Autoforhandling"
1GFD                    = "1.0 Gbps full dupleks"
10MHD		  	= "10 Mbps halv dupleks"
10MFD		  	= "10 Mbps full dupleks"
100MHD			= "100 Mbps halv dupleks"
100MFD			= "100 Mbps full dupleks"
WakeUpCapabilities      = "Oppvåkingsmuligheter"
None            	= "Ingen"
LinkChange	        = "Forbindelsesendring"
MagicPacket	        = "Magic Packet"
PatternMatch	        = "Mønstergjenkjenning"
Link_Magic      	= "Forbindelsesendring og MagicPacket"
Link_Pattern    	= "Forbindelsesendring og mønstergjenkjenning"
Magic_Pattern   	= "MagicPacket og mønstergjenkjenning"
All             	= "Alle"
On              	= "På"
Off             	= "Av"
TXEna 			= "Tx aktivert"
RXEna 			= "Rx aktivert"
TXRXEna 		= "Tx og Rx aktivert"
IPChksumOffv4 		= "IPv4-sjekksumavlasting"
TCPChksumOffv4 		= "TCP-sjekksumavlasting (IPv4)"
UDPChksumOffv4 		= "UDP-sjekksumavlasting (IPv4)"
LsoOff                  = "Avlasting ved stor sending"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Polish
[Strings.0415]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Ramka Jumbo"
2KBMTU      		= "MTU 2 KB"
3KBMTU      		= "MTU 3 KB"
4KBMTU      		= "MTU 4 KB"
5KBMTU      		= "MTU 5 KB"
6KBMTU      		= "MTU 6 KB"
7KBMTU      		= "MTU 7 KB"
8KBMTU      		= "MTU 8 KB"
9KBMTU      		= "MTU 9 KB"
APSmode			= "Tryb APS"
AZPower                 = "802.3az"
NetAddr         	= "Adres sieciowy"
MTU             	= "Maksymalny rozmiar ramki"
TOff            	= "Odciążanie zadań"
MaxIrq          	= "Maks. IRQ na sekundę"
NumRx           	= "Liczba buforów Rx"
NumTx           	= "Liczba buforów Tx"
FlowCtrl        	= "Sterowanie przepływem"
ShutDW          	= "Wyłączanie i budzenie"
MediaType       	= "Typ nośnika"
Auto		  	= "Automatyczna negocjacja"
1GFD                    = "1.0 Gb/s pełny dupleks"
10MHD		  	= "10 Mb/s, półdupleks"
10MFD		  	= "10 Mb/s, pełny dupleks"
100MHD			= "100 Mb/s, półdupleks"
100MFD			= "100 Mb/s, pełny dupleks"
WakeUpCapabilities      = "Funkcje budzenia"
None            	= "Brak"
LinkChange	        = "Zmiana łącza"
MagicPacket	        = "Pakiet specjalny"
PatternMatch	        = "Dopasowanie do wzorca"
Link_Magic      	= "Zmiana łącza i pakiet specjalny"
Link_Pattern    	= "Zmiana łącza i dopasowanie do wzorca"
Magic_Pattern   	= "Pakiet specjalny i dopasowanie do wzorca"
All             	= "Wszystko"
On              	= "Włączone"
Off             	= "Wyłączone"
TXEna 			= "Tx włączone"
RXEna 			= "Rx włączone"
TXRXEna 		= "Tx i Rx włączone"
IPChksumOffv4 		= "Odciążanie sumy kontrolnej IPv4"
TCPChksumOffv4 		= "Odciążanie sumy kontrolnej TCP (IPv4)"
UDPChksumOffv4 		= "Odciążanie sumy kontrolnej UDP (IPv4)"
LsoOff                  = "Odciążanie dużych transmisji"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Russian
[Strings.0419]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Кадры крупных размеров"
2KBMTU      		= "2 Кб MTU"
3KBMTU      		= "3 Кб MTU"
4KBMTU      		= "4 Кб MTU"
5KBMTU      		= "5 Кб MTU"
6KBMTU      		= "6 Кб MTU"
7KBMTU      		= "7 Кб MTU"
8KBMTU      		= "8 Кб MTU"
9KBMTU      		= "9 Кб MTU"
APSmode			= "Режим APS"
AZPower                 = "802.3az"
NetAddr         	= "Сетевой адрес"
MTU             	= "Максимальный размер кадра"
TOff            	= "Разгрузка операций задачи"
MaxIrq          	= "Макс. IRQ в секунду"
NumRx           	= "Число буферов приема"
NumTx           	= "Число буферов передачи"
FlowCtrl        	= "Управление потоком"
ShutDW          	= "Завершение Пробуждение"
MediaType       	= "Тип носителя"
Auto		  	= "Автосогласование"
1GFD                    = "1000 Мбит/с, полный дуплекс"
10MHD		  	= "10 Мбит/с, полудуплекс"
10MFD		  	= "10 Мбит/с, полный дуплекс"
100MHD			= "100 Мбит/с, полудуплекс"
100MFD			= "100 Мбит/с, полный дуплекс"
WakeUpCapabilities      = "Возможности пробуждения"
None            	= "Нет"
LinkChange	        = "Смена связи"
MagicPacket	        = "Пакет Magic"
PatternMatch	        = "Соответствие шаблону"
Link_Magic      	= "Смена связи и Пакет Magic"
Link_Pattern    	= "Смена связи и соответствие шаблону"
Magic_Pattern   	= "Пакет Magic и соответствие шаблону"
All             	= "Все"
On              	= "Вкл."
Off             	= "Выкл."
TXEna 			= "Передача включена"
RXEna 			= "Прием включен"
TXRXEna 		= "Передача и прием включены"
IPChksumOffv4 		= "Разгрузка операций контрольной суммы IPv4"
TCPChksumOffv4 		= "Разгрузка операций контрольной суммы ТСР (IPv4)"
UDPChksumOffv4 		= "Разгрузка операций контрольной суммы UDP (IPv4)"
LsoOff                  = "Разгрузка операций с отправкой больших пакетов"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Slovak
[Strings.041b]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Rámec Jumbo"
2KBMTU      		= "2 kB MTU"
3KBMTU      		= "3 kB MTU"
4KBMTU      		= "4 kB MTU"
5KBMTU      		= "5 kB MTU"
6KBMTU      		= "6 kB MTU"
7KBMTU      		= "7 kB MTU"
8KBMTU      		= "8 kB MTU"
9KBMTU      		= "9 kB MTU"
APSmode			= "Režim APS"
AZPower                 = "802.3az"
NetAddr         	= "Sieťová adresa"
MTU             	= "Maximálna veľkosť rámca"
TOff            	= "Zníženie záťaže pri vykonávaní úlohy"
MaxIrq          	= "Max. počet prerušení IRQ za sekundu"
NumRx           	= "Veľkosť medzipamäte pre príjem"
NumTx           	= "Veľkosť medzipamäte pre odosielanie"
FlowCtrl        	= "Riadenie toku"
ShutDW          	= "Vypnutie/prebudenie"
MediaType       	= "Typ média"
Auto		  	= "Automatické vyjednávanie"
1GFD                    = "Úplný duplex 1.0 Gb/s"
10MHD		  	= "Polovičný duplex 10 Mb/s"
10MFD		  	= "Úplný duplex 10 Mb/s"
100MHD			= "Polovičný duplex 100 Mb/s"
100MFD			= "Úplný duplex 100 Mb/s"
WakeUpCapabilities      = "Možnosti prebudenia"
None            	= "Žiadne"
LinkChange	        = "Zmena linky"
MagicPacket	        = "Magický paket"
PatternMatch	        = "Zhoda vzorov"
Link_Magic      	= "Zmena linky a magický paket"
Link_Pattern    	= "Zmena linky a zhoda vzorov"
Magic_Pattern   	= "Magický paket a zhoda vzorov"
All             	= "Všetko"
On              	= "Zap."
Off             	= "Vyp."
TXEna 			= "Odosielanie povolené"
RXEna 			= "Príjem povolený"
TXRXEna 		= "Príjem a odosielanie povolené"
IPChksumOffv4 		= "Zníženie záťaže pri kontrolných súčtoch protokolu IPv4"
TCPChksumOffv4 		= "Zníženie záťaže pri kontrolných súčtoch protokolu TCP (IPv4)"
UDPChksumOffv4 		= "Zníženie záťaže pri kontrolných súčtoch protokolu UDP (IPv4)"
LsoOff                  = "Zníženie záťaže pri odosielaní veľkého množstva údajov"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Swedish
[Strings.041d]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumboram"
2KBMTU      		= "2 kB MTU"
3KBMTU      		= "3 kB MTU"
4KBMTU      		= "4 kB MTU"
5KBMTU      		= "5 kB MTU"
6KBMTU      		= "6 kB MTU"
7KBMTU      		= "7 kB MTU"
8KBMTU      		= "8 kB MTU"
9KBMTU      		= "9 kB MTU"
APSmode			= "APS-läge"
AZPower                 = "802.3az"
NetAddr         	= "Nätverksadress"
MTU             	= "Maximal ramstorlek"
TOff            	= "Uppgiftsavlastning"
MaxIrq          	= "Max IRQ per sekund"
NumRx           	= "Antal Rx-buffertar"
NumTx           	= "Antal Tx-buffertar"
FlowCtrl        	= "Flödeskontroll"
ShutDW          	= "Avstängning, väckning"
MediaType       	= "Medietyp"
Auto		  	= "Automatisk förhandling"
1GFD                    = "1.0 Gbit/s full duplex"
10MHD		  	= "10 Mbit/s halv duplex"
10MFD		  	= "10 Mbit/s full duplex"
100MHD			= "100 Mbit/s halv duplex"
100MFD			= "100 Mbit/s full duplex"
WakeUpCapabilities      = "Väckningsfunktioner"
None            	= "Inget"
LinkChange	        = "Länkändring"
MagicPacket	        = "Magiskt paket"
PatternMatch	        = "Mönstermatchning"
Link_Magic      	= "Länkändring och magiskt paket"
Link_Pattern    	= "Länkändring och mönstermatchning"
Magic_Pattern   	= "Magiskt paket och mönstermatchning"
All             	= "Allt"
On              	= "På"
Off             	= "Av"
TXEna 			= "Tx-aktiverad"
RXEna 			= "Rx-aktiverad"
TXRXEna 		= "Tx- och Rx-aktiverad"
IPChksumOffv4 		= "IPv4-kontrollsummeavlastning"
TCPChksumOffv4 		= "TCP-kontrollsummeavlastning (IPv4)"
UDPChksumOffv4 		= "UDP-kontrollsummeavlastning (IPv4)"
LsoOff                  = "Avlastning för stor sändning"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Turkish
[Strings.041f]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "Jumbo Çerçeve"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS modu"
AZPower                 = "802.3az"
NetAddr         	= "Ağ Adresi"
MTU             	= "Maksimum Çerçeve Boyutu"
TOff            	= "Görev Boşaltma"
MaxIrq          	= "Maks IRQ/Saniye"
NumRx           	= "Rx Arabelleklerinin sayısı"
NumTx           	= "Tx Arabelleklerinin sayısı"
FlowCtrl        	= "Akış Denetimi"
ShutDW          	= "Kapatma Uyandırma"
MediaType       	= "Ortam Türü"
Auto		  	= "Otomatik Anlaşma"
1GFD                    = "1.0 Gbps Tam Çift Yönlü"
10MHD		  	= "10 Mbps Yarı Çift Yönlü"
10MFD		  	= "10 Mbps Tam Çift Yönlü"
100MHD			= "100 Mbps Yarı Çift Yönlü"
100MFD			= "100 Mbps Tam Çift Yönlü"
WakeUpCapabilities      = "Uyandırma Yetenekleri"
None            	= "Hiçbiri"
LinkChange	        = "Bağlantı Değişikliği"
MagicPacket	        = "Sihirli Paket"
PatternMatch	        = "Desen Eşleştirme"
Link_Magic      	= "Bağlantı Değişikliği ve Sihirli Paket"
Link_Pattern    	= "Bağlantı Değişikliği ve Desen Eşleştirme"
Magic_Pattern   	= "Sihirli Paket ve Desen Eşleştirme"
All             	= "Tümü"
On              	= "Açık"
Off             	= "Kapalı"
TXEna 			= "Tx Etkin"
RXEna 			= "Rx Etkin"
TXRXEna 		= "Tx ve Rx Etkin"
IPChksumOffv4 		= "IPv4 Sağlama Toplamı Boşaltma"
TCPChksumOffv4 		= "TCP Sağlama Toplamı Boşaltma (IPv4)"
UDPChksumOffv4 		= "UDP Sağlama Toplamı Boşaltma (IPv4)"
LsoOff                  = "Büyük Gönderme Boşaltması"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Arabic (Saudi Arabia)
[Strings.0401]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros                 = "Atheros"
JumboFrame  		= "ار الجامبو"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "وضع APS"
AZPower                 = "802.3az"
NetAddr         	= "عنوان الشبكة"
MTU             	= "الحد الأقصى حجم الإطار"
TOff            	= "تفريغ المهمة"
MaxIrq          	= "الحد الأقصى لـ IRQ في الثانية"
NumRx           	= "عدد حواجز Rx"
NumTx           	= "عدد حواجز Tx"
FlowCtrl		= "تحكم التدفق"
ShutDW			= "ايقاظ إيقاف التشغيل"
MediaType       	= "نوع الوسائط"
Auto		  	= "تفاوض تلقائي"
1GFD                    = "1000 ميجابايت في الثانية ازدواج كامل"
10MHD		  	= "10 ميجابايت في الثانية نصف ازدواج"
10MFD		  	= "10 ميجابايت في الثانية ازدواج كامل"
100MHD			= "ميجابايت في الثانية نصف ازدواج 100"
100MFD			= "100 ميجابايت في الثانية ازدواج كامل"
WakeUpCapabilities      = "قدرات الايقاظ"
None            	= "بلا"
LinkChange	        = "تغيير الارتباط"
MagicPacket	        = "حزمة سحرية"
PatternMatch	        = "توافق النمط"
Link_Magic      	= "تغيير الارتباط & حزمة سحرية"
Link_Pattern    	= "تغيير الارتباط & توافق النمط"
Magic_Pattern   	= "حزمة سحرية & توافق النمط"
All             	= "الكل"
On              	= "تشغيل"
Off             	= "إيقاف"
TXEna 			= "Tx ممكن"
RXEna 			= "Rx ممكن"
TXRXEna 		= "Tx & Rx ممكن"
IPChksumOffv4 		= "تفريغ IPv4 Checksum"
TCPChksumOffv4 		= "تفريغ TCP Checksum (IPv4)"
UDPChksumOffv4 		= "تفريغ UDP Checksum (IPv4)"
LsoOff                  = "تفريغ إرسال كبير"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Croatian
[Strings.041a]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros 		= "Atheros"
JumboFrame  		= "Jumbo okvir"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS način rada"
AZPower                 = "802.3az"
NetAddr         	= "Adresa mreže"
MTU             	= "Maksimalna veličina okvira"
TOff            	= "Iskrcavanje zadatka"
MaxIrq          	= "Maks IRQ na sekundu"
NumRx           	= "Broj Rx međumemorija"
NumTx           	= "Broj Tx međumemorija"
FlowCtrl		= "Nadzor protoka"
ShutDW			= "Buđenje gašenja"
MediaType       	= "Vrsta medija"
Auto		  	= "Samostalno pregovaranje"
1GFD                    = "1.0 Gbps puni dupleks"
10MHD		  	= "10 Mbps polu dupleks"
10MFD		  	= "10 Mbps puni dupleks"
100MHD			= "100 Mbps polu dupleks"
100MFD			= "100 Mbps puni dupleks"
WakeUpCapabilities      = "Mogućnosti buđenja"
None            	= "Nijedan"
LinkChange	        = "Promjena veze"
MagicPacket	        = "Čaroban paket"
PatternMatch	        = "Podudaranje s uzorcem"
Link_Magic      	= "Promjenaveze & Čarobanpaket"
Link_Pattern    	= "Promjenaveze & Podudaranjesuzorcem"
Magic_Pattern   	= "Čarobanpaket & Podudaranjesuzorcem"
All             	= "Svi"
On              	= "Uključeno"
Off             	= "Isključeno"
TXEna 			= "Tx aktiviran"
RXEna 			= "Rx aktiviran"
TXRXEna 		= "Tx & Rx aktivirani"
IPChksumOffv4 		= "Iskrcavanje IPv4 zbroja za provjeru"
TCPChksumOffv4 		= "Iskrcavanje TCP zbroja za provjeru (IPv4)"
UDPChksumOffv4 		= "Iskrcavanje UDP zbroja za provjeru (IPv4)"
LsoOff                  = "Iskrcavanje velikog slanja"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Hebrew
[Strings.040d]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros 		= "Atheros"
JumboFrame  		= "מסגרת ענקית"
2KBMTU      		= "2 ק''ב MTU (יחידת שליחה מירבית)"
3KBMTU      		= "3 ק''ב MTU"
4KBMTU      		= "4 ק''ב MTU"
5KBMTU      		= "5 ק''ב MTU"
6KBMTU      		= "6 ק''ב MTU"
7KBMTU      		= "7 ק''ב MTU"
8KBMTU      		= "8 ק''ב MTU"
9KBMTU      		= "9 ק''ב MTU"
APSmode			= "מצב APS"
AZPower                 = "802.3az"
NetAddr         	= "כתובת רשת"
MTU             	= "מספר פריימים מירבי"
TOff            	= "שחרור משימה"
MaxIrq          	= "IRQ (בקשת הפרעה) מירביות בשניה"
NumRx           	= "מספר בופרי Rx"
NumTx           	= "מספר בופרי Tx"
FlowCtrl		= "בקרת תנועה"
ShutDW			= "התעוררות ממצב כבוי"
MediaType       	= "סוג מדיה"
Auto		  	= "מו''מ אוטומטי"
1GFD                    = "דופלקס מלא 1000 מ''ב/שנייה"
10MHD		  	= "חצי דופלקס 10 מ''ב/שנייה"
10MFD		  	= "דופלקס מלא 10 מ''ב/שנייה"
100MHD			= "חצי דופלקס 100 מ''ב/שנייה"
100MFD			= "דופלקס מלא 100 מ''ב/שנייה"
WakeUpCapabilities      = "יכולות התעוררות"
None            	= "ללא"
LinkChange	        = "שינוי חיבור"
MagicPacket	        = "פאקטת קסם (Magic Packet)"
PatternMatch	        = "התאמת תבנית"
Link_Magic      	= "פאקטת קסם שינוי חיבור"
Link_Pattern    	= "התאמת תבניתשינוי חיבור"
Magic_Pattern   	= "התאמת תבנית ופאקטת קסם"
All             	= "הכל"
On              	= "פעיל"
Off             	= "כבוי"
TXEna 			= "הפעל Tx"
RXEna 			= "הפעל Rx"
TXRXEna 		= "הפעל Tx ו-Rx"
IPChksumOffv4 		= "שחרור סיכום ביקורת IPv4"
TCPChksumOffv4 		= "שחרור סיכום ביקורת TCP (IPv4)"
UDPChksumOffv4 		= "שחרור סיכום ביקורת UDP (IPv4)"
LsoOff                  = "שליחת שחרור גדולה"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Portuguese (Portugal)
[Strings.0816]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros 		= "Atheros"
JumboFrame  		= "Trama jumbo"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "Modo APS"
AZPower                 = "802.3az"
NetAddr         	= "Endereço de rede"
MTU             	= "Tamanho de estrutura máximo"
TOff            	= "Descarregar tarefa"
MaxIrq          	= "Máx. IRQ por segundo"
NumRx           	= "Número de memórias intermédias Rx"
NumTx           	= "Número de memórias intermédias Tx"
FlowCtrl		= "Controlo de fluxo"
ShutDW			= "Fechar despertar"
MediaType       	= "Tipo de média"
Auto		  	= "Negociação auto"
1GFD                    = "1.0 Gbps cheio duplex"
10MHD		  	= "10 Mbps meio duplex"
10MFD		  	= "10 Mbps cheio duplex"
100MHD			= "100 Mbps meio duplex"
100MFD			= "100 Mbps cheio duplex"
WakeUpCapabilities      = "Capacidades despertar"
None		        = "Nenhum"
LinkChange	        = "Alteração de ligação"
MagicPacket	        = "Pacote mágico"
PatternMatch	        = "Combinação padrão"
Link_Magic      	= "Alteração de ligação e Pacote mágico"
Link_Pattern    	= "Alteração de ligação e Combinação padrão"
Magic_Pattern   	= "Pacote mágico e Combinação padrão"
All             	= "Todos"
On              	= "Ligar"
Off             	= "Desligar"
TXEna 			= "Tx activado"
RXEna 			= "Rx activado"
TXRXEna 		= "Tx e Rx activado"
IPChksumOffv4 		= "Descarregar teste por soma IPv4"
TCPChksumOffv4 		= "Descarregar teste por soma TCP (IPv4)"
UDPChksumOffv4 		= "Descarregar teste por soma UDP (IPv4)"
LsoOff                  = "Descarregar envio grande"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Romanian
[Strings.0418]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros 		= "Atheros"
JumboFrame  		= "Unitate digitală mare de transmitere date"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "Mod APS"
AZPower                 = "802.3az"
NetAddr         	= "Adresă Reţea"
MTU             	= "Dimensiunea maximă a unităţii digitale de transmitere date"
TOff            	= "Transfer Sarcină"
MaxIrq          	= "Max IRQ pe secundă"
NumRx           	= "Numărul Memoriilor Rx"
NumTx           	= "Numărul Memoriilor Tx"
FlowCtrl		= "Control Transmitere Date"
ShutDW			= "Oprire Pornire"
MediaType       	= "Tip Suport"
Auto		  	= "Auto Negociere"
1GFD                    = "1.0 Gbps Duplex Complet"
10MHD		  	= "10 Mbps Semi Duplex"
10MFD		  	= "10 Mbps Duplex Complet"
100MHD			= "100 Mbps Semi Duplex"
100MFD			= "100 Mbps Duplex Complet"
WakeUpCapabilities      = "Capabilităţi Pornire"
None		        = "Nimic"
LinkChange	        = "Schimbare Legătură"
MagicPacket	        = "Pachet Magic"
PatternMatch	        = "Potrivire Model"
Link_Magic      	= "SchimbareLegătură & PachetMagic"
Link_Pattern    	= "SchimbareLegătură & PotrivireModel"
Magic_Pattern   	= "PachetMagic & PotrivireModel"
All             	= "Toate"
On              	= "Pornit"
Off             	= "Oprit"
TXEna 			= "Tx Activat"
RXEna 			= "Rx Activat"
TXRXEna 		= "Tx & Rx Activat"
IPChksumOffv4 		= "Transfer Date IPv4"
TCPChksumOffv4 		= "Transfer Date TCP (IPv4)"
UDPChksumOffv4 		= "Transfer Date UDP (IPv4)"
LsoOff                  = "Transfer Mare"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."

; Slovenian
[Strings.0424]
;; Translation from this point ON.
;---------------------------------------------------------------------------------------------------
Atheros			= "Atheros"
JumboFrame  		= "Veliki okvir"
2KBMTU      		= "2KB MTU"
3KBMTU      		= "3KB MTU"
4KBMTU      		= "4KB MTU"
5KBMTU      		= "5KB MTU"
6KBMTU      		= "6KB MTU"
7KBMTU      		= "7KB MTU"
8KBMTU      		= "8KB MTU"
9KBMTU      		= "9KB MTU"
APSmode			= "APS način"
AZPower                 = "802.3az"
NetAddr         	= "Omrežni naslovi"
MTU             	= "Maksimalna velikost okvirja"
TOff            	= "Razbremenitev naloge"
MaxIrq          	= "Maks IRQ na sekundo"
NumRx           	= "Število Rx medpomnilnikov"
NumTx           	= "Število Tx medpomnilnikov"
FlowCtrl		= "Kontrola pretoka"
ShutDW			= "Bujenje po izklopu"
MediaType       	= "Vrsta medija"
Auto		  	= "Samodejno pogajanje"
1GFD                    = "1.0 Gbps polni dupleks"
10MHD		  	= "10 Mbps polovični dupleks"
10MFD		  	= "10 Mbps polni dupleks"
100MHD			= "100 Mbps polovični dupleks"
100MFD			= "100 Mbps polni dupleks"
WakeUpCapabilities      = "Zmožnosti bujenja"
None		        = "Brez"
LinkChange	        = "Sprememba povezave"
MagicPacket	        = "Magični paket"
PatternMatch	        = "Enak vzorec"
Link_Magic      	= "Sprememba povezave in Magični paket"
Link_Pattern    	= "Sprememba povezave in Enak vzorec"
Magic_Pattern   	= "Magični paket in Enak vzorec"
All             	= "Vse"
On              	= "Vklopljeno"
Off             	= "Izklopljeno"
TXEna 			= "Tx omogočeno"
RXEna 			= "Rx omogočeno"
TXRXEna 		= "Tx in Rx omogočeno"
IPChksumOffv4 		= "IPv4 kontrolna vsota razbremenitve"
TCPChksumOffv4 		= "TCP kontrolna vsota razbremenitve (IPv4)"
UDPChksumOffv4 		= "UDP kontrolna vsota razbremenitve (IPv4)"
LsoOff                  = "Razbremenitev velikega pošiljanja"
VLanID                  = "VLAN ID"

Atheros.L1c  		= "Atheros AR8131 PCI-E Gigabit Ethernet Controller"
Atheros.L1cd  		= "Atheros AR813x/815x PCI-E Gigabit Ethernet Controller"
Atheros.L2c  		= "Atheros AR8132 PCI-E Fast Ethernet Controller"
Atheros.L1d  		= "Atheros AR8151 PCI-E Gigabit Ethernet Controller"
Atheros.L2cb  		= "Atheros AR8152/8158 PCI-E Fast Ethernet Controller"
L1c.Service.DispName 	= "NDIS Miniport Driver for Atheros AR813x/AR815x PCI-E Ethernet Controller"
DriverDisk		= "Atheros AR81xx Series PCI-E Ethernet Controller Installation Disk"
HelpText		= "This Atheros network Controller connects you to the network."